88::


36:
The %s instruction can't be\n
executed while the system is\n
in a stop state

37:
The object that the\n
instruction %s,\n
was waiting for has been\n
dropped

38:
Rerun the instruction

39:
The instruction %s, was\n
interrupted, reason unknown

40:
User frame error\n
Not possible to get the coordinated\n
user frame

41:
No single number defined

42:
Axes error\n
The single axis is not init correctly

43:
Another %s instruction is\n
waiting for the object

44:
Another %s instruction is\n
waiting for a distance to\n
the object

45:
The %s instruction has\n
lost contact with the\n
conveyor.

46:
 mech unit is not a single


47:
The sensor process is not\n
init correctly

48:
The sensor is not activated

49:
The conveyor is not activated

50:
The %s instruction is already connected

51:
The parameter %s is negative

52:
Set it positive or to zero

53:
The parameter %s forces the\n
robot out of workspace

54:
Decrease the value


