%%%
  VERSION: 1
  LANGUAGE: ENGLISH
%%%

MODULE STTEXT (SYSMODULE)

  ! Description: 
  ! CONST string Version_XXXXXXXX := "1.2";
  !
  !          XXXXXXXX - Module name
  !                 1 - version number  (changed of SEROP) 
  !                 2 - revision number (changed of SEROP)
  CONST string Version_STTEXT := "4.0";

  ! Error messages - servo gun
  CONST string TxtErrGunTitle := 	"Gun error";
  CONST string TxtErrCloseSgun :=	"Can not close the gun in motors off";
  CONST string TxtErrOpenSgun :=	"Can not open the gun in motors off";
  CONST string TxtErrCalibSgun :=	"Can not calibrate the gun in motors off";
  CONST string TxtErrNoName := 		"Name not specified in data(mecunit)";
  CONST string TxtErrMecNoAct := 	"Mechanical unit is not active";
  CONST string TxtGunNotOpen :=		"Can not close the gun. It is not open!";
  CONST string TxtServCal1 := 		"A ManServiceCalib is required before";
  CONST string TxtServCal2 := 		"continuing the program execution.";

  ! Function keys messages
  CONST string TxtCancel := 		"Cancel";
  CONST string TxtRetry := 		"Retry";
  CONST string TxtIgnore:=		"Ignore";
  CONST string TxtOK :=             	"OK";

  ! Error messages - plate thickness error
  CONST string TxtGenCurrGun := 	"Current gun: ";
  CONST string TxtPlateGunPos :=	"Negative gun position!";
  CONST string TxtPlateMissing :=	"Missing plates!";
  CONST string TxtPlateImproper :=	"Improper geometry!";
  CONST string TxtPlateTol :=		"Tolerance:          ";
  CONST string TxtPlateExpTh :=		"Expected thickness: ";
  CONST string TxtPlateAchTh :=		"Achieved thickness: ";
  CONST string TxtInfoTP	 :=	"Press Ignore to skip the thickness test";
  CONST string TxtContAnyWay :=		"Press OK to close the gun";
  CONST string TxtCurrErrAbort :=	"Current error ignored";

  ! Teachpendant messages used in routine ManCalib
  CONST string TxtManCalibCh := 	"Choose the type of calibration";

  ! Teachpendant messages used in routine ManServiceCalib
  CONST string TxtManServCalib := 	"Service calibration";
  CONST string TxtRevCUpdate := 	"1.Synchronize the tip position.";
  CONST string TxtManRevCUpdate := 	"After revolution counter update";
  CONST string TxtFineCalib := 		"2.Initialize the servo gun position.";
  CONST string TxtManFineCalib := 	"After the gun has been fine calibrated.";

  ! Teachpendant messages used in routine ManForceCalib
  CONST string TxtManForceCal := 	"Manual force calibration";
  CONST string TxtManSelNum := 		"How many measurements? (min2,max10)";
  CONST string TxtManSelVal := 		"Enter force value";
  CONST string TxtManSelThick :=	"Select sensor thickness (min0,max100)";
  CONST string TxtManSelTime :=		"Select force time (min1,max10)";
  CONST string TxtManSelOK := 		"Press OK to continue";
  CONST string TxtManSelCancel := 	"Press CANCEL to change";
  CONST string TxtManSetThick :=	"Enter thickness in mm.";
  CONST string TxtManSetTime :=		"Enter time in sec.";
  CONST string TxtManInvVal := 		"Invalid value, default will be used:";
  CONST string TxtManInValue := 	"Enter measured tip force";
  CONST string TxtManNoCalib := 	"Number of force calibrations done: ";
  CONST string TxtManNoCalibP := 	"No of calibrations to be performed ";
  CONST string TxtManMaxForce :=	"Select max tip force";
  CONST string TxtManNumCalib :=	"Select number of calibrations";
  CONST string TxtManCurrCalib1 :=	"Press OK to perform";
  CONST string TxtManCurrCalib2 :=	"calibration no: ";
  CONST string TxtManCurrTorque := 	"Current motor torque = ";
  CONST string TxtManCurrForce := 	"Current force = ";
  CONST string TxtManCurrThick := 	"Current thickness = ";
  CONST string TxtManCurrTime := 	"Current force time = ";
  CONST string TxtManCurrValue := 	"Current value: ";
  CONST string TxtManCurrVal := 	"Current values:";
  CONST string TxtManQueryAct1 := 	"Press OK to activate";
  CONST string TxtManQueryAct2 := 	"the new calibration";
  CONST string TxtManMaxProgF1 := 	"Max programmable force";
  CONST string TxtManMaxProgF2 := 	"for this gun is ";
  CONST string TxtManAcceptVal :=   	"Is this value OK?";
  CONST string TxtManAckMeas   :=  	"Press OK to accept measurement";
  CONST string TxtManRedoMeas  :=  	"Press retry to try again";

ENDMODULE