80::
0:
Communication
1:
Serial Channel
2:
Name
3:
Baud rate
4:
Parity
5:
No of bits
6:
No stop bits
7:
Protocol
8:
Local IP Address
9:
Remote IP Address
10:
7
11:
8
12:
1
13:
2
14:
SLIP
15:
XONXOFF
16:
NONE
17:
300
18:
600
19:
1200
20:
2400
21:
4800
22:
9600
23:
19200
24:
38400
25:
none
26:
odd
27:
even
28:
ignore
29:
Name     Channel      Baudrate
30:
Channel
31:
Physical Channels
32:
Transmission Protocols
33:
Application Protocols
34:
Type
35:
PhyChannel
36:
PortNo
37:
Name        Connector
38:
Name        Type        PhyChannel
39:
Name        Type        Trans Prot.
40:
Trans Prot.
41:
Send start-up msg
42:
TRUE
43:
FALSE
44:
on
45:
off
46:
Flow Control
47:
Server IP Addr
48:
Mount All
49:
Trusted
50:
Local Path
51:
Server Path
52:
User ID
53:
Group ID
54:
Yes
55:
No
56:
Show on TPU
57:
Gateway
58:
Subnet mask
59:
Duplex
60:
Full
61:
Half
62:
Enable SUBSCW
63:
Username
64:
Password
65:
Connector
66:
None
67:
RTS/CTS
68:
XON/XOFF
69:
MaxFileSize kB
