27::
0:
V/V a komunikace
1000:
Nazev sbern. neni platny\n
Popis\Duvod:\n
- Ovladac %s: ma neplatny nazev sbernice\n
\t\n
Seznam kontrol:\n
1. Zmente nazev sbernice pro ovladac
1001:
Zdvojena adresa\n
Popis\Duvod:\n
- Stejna adresa pro jednotku %s a %s\n
\t\n
Seznam kontrol:\n
1.Zkontrolujte adresu\n
2.Zkontrolujte sbernici
1002:
Neplatny ovladac\n
Popis\Duvod:\n
- Jednotka %s: ma nespecifik. ovladac\n
\t\n
Seznam kontrol:\n
1.Zkontrolujte ovladace proti ovladaci\n
  specifikovanemu pro jednotku
1003:
Neplatna jednotka\n
Popis\Duvod:\n
- Jednotka specifikovana pro signal %s\n
  neni v sekci jednotky specifikovana\n
\t\n
Seznam kontrol:\n
1.Zmente nazev jednotky\n
2.Na seznam jednotek pridejte novou jedn
1004:
Neplatna delka signalu\n
Popis\Duvod:\n
- Delka digitalniho signalu\n
  %s musi byt 1\n
\t\n
Seznam kontrol:\n
1.Zmente delku na 1 nebo odstrante\n
  prikaz.
1005:
Neplatny cas filtru\n
Popis\Duvod:\n
- Signal %s: Cas pasivniho filtru\n
  by mel byt 0 nebo %d - %d ms\n
\t\n
Seznam kontrol:\n
1.Zmente cas filtru
1006:
Neplatny cas filtru\n
Popis\Duvod:\n
- Signal %s: Cas aktivniho filtru\n
  by mel byt 0 nebo %d - %d ms\n
\t\n
Seznam kontrol:\n
1.Zmente cas filtru
1007:
Logic. hodn. mimo rozsah\n
Popis\Duvod:\n
- Signal %s: logicke max je mensi nebo\n
  rovne logickemu min\n
\t\n
Seznam kontrol:\n
1.Opravte hodnoty, aby max bylo vetsi\n
  nez min
1008:
Fyz. hodn. mimo rozsah\n
Popis\Duvod:\n
- Signal %s: fyzicke max je mensi nebo\n
  rovne fyzickemu min\n
\t\n
Seznam kontrol:\n
1.Opravte hodnoty, aby max bylo vetsi\n
  nez min
1009:
Neplatny typ\n
Popis\Duvod:\n
- Signal %s: typ signalu\n
  neni platny\n
\t\n
Seznam kontrol:\n
1.Zmente typ
1010:
Signal mimo rozsah\n
Popis\Duvod:\n
- Signal %s: cislo fyzickeho signalu\n
  + delka -1 je > %d\n
\t\n
Seznam kontrol:\n
1.Zmente cislo fyzickeho signalu\n
2.Zmente delku
1015:
Preteceni digital. vstupu\n
Popis\Duvod:\n
- Pocet digitalnich vstupnich kanalu\n
  pro desku %s je vetsi\n
  nez %d\n
\t\n
Seznam kontrol:\n
1. Snizte pocet digitalnich vstupu
1016:
Preteceni digit. vystupu\n
Popis\Duvod:\n
- Pocet digitalnich vystupnich signalu\n
  pro desku %s je vetsi\n
  nez %d\n
\t\n
Seznam kontrol:\n
1. Snizte pocet digitalnich vystupu
1017:
Zadny aktivacni signal\n
Popis\Duvod:\n
- Chybi aktivacni signal pro propojeni\n
\t\n
Seznam kontrol:\n
1. Musi byt zadan jeden aktivacni signal
1018:
Preteceni aktiv. signalu\n
Popis\Duvod:\n
-Pocet aktivacnich signalu pro\n
 propojeni je prilis velky\n
\t\n
Seznam kontrol:\n
1. Musi byt zadan pouze jeden aktivacni\n
   signal
1019:
Chybi definice signalu\n
Popis\Duvod:\n
-Signal: %s, v krizi neni definovan\n
\t\n
Seznam kontrol:\n
1. Definujte nazev signalu\n
   v sekci signalu
1020:
Zadny signal vysledku\n
Popis\Duvod:\n
- Chybi signal vysledku\n
\t\n
Seznam kontrol:\n
1. Musi byt zadan alespon jeden signal\n
   vysledku
1021:
Zdvojene krizove signaly\n
Popis\Duvod:\n
- Signal: %s, existuje jako OD\n
  i jako DO.\n
\t\n
Seznam kontrol:\n
1. Pro OD a pro DO nelze zadat stejny\n
   signal
1022:
Fyz. max je prilis vysoke\n
Popis\Duvod:\n
- Signal: %s\n
- Fyzicka max hodnota > %d\n
\t\n
Seznam kontrol:\n
1. Zmente hodnotu v konfiguraci
1023:
Fyz. min je prilis nizke\n
Popis\Duvod:\n
- Signal: %s\n
- Fyzicka min hodnota < %d\n
\t\n
Seznam kontrol:\n
1. Zmente hodnotu v konfiguraci
1024:
Fyz. hodn. prilis vysoka\n
Popis\Duvod:\n
- Signal: %s\n
- Soucasna hodnota = %d > Maxhodn = %d\n
- Hodnota nastavena na Maxhodn\n
\t\n
Seznam kontrol:\n
1. Zmente fyzickou max hodnotu\n
   v konfiguraci
1025:
Fyz. hodnota prilis nizka\n
Popis\Duvod:\n
- Signal: %s\n
- Soucasna hodnota = %d < Minhodn = %d\n
- Hodnota nastavena na Minhodn\n
\t\n
Seznam kontrol:\n
1. Zmente fyzickou min hodnotu\n
   v konfiguraci
1026:
Log. hodn. prilis vysoka\n
Popis\Duvod:\n
- Signal: %s\n
- Soucasna hodnota = %d > Maxhodn = %d\n
- Hodnota nastavena na Maxhodn\n
\t\n
Seznam kontrol:\n
1. Zmente logickou max hodnotu\n
   v konfiguraci
1027:
Log. hodnota prilis nizka\n
Popis\Duvod:\n
- Signal: %s\n
- Soucasna hodnota = %d < Minhodn = %d\n
- Hodnota nastavena na Minhodn\n
\t\n
Seznam kontrol:\n
1. Zmente logickou min hodnotu\n
   v konfiguraci
1033:
Digit. vstup mimo rozsah\n
Popis\Duvod:\n
- Pocet digitalnich vstupu je mimo\n
  rozsah desky s adresou %d\n
  max pocet vstupu je %d\n
\t\n
Seznam kontrol:\n
1. Zmente konfiguraci pro tuto desku
1034:
Digit. vystup mimo rozsah\n
Popis\Duvod:\n
- Pocet digitalnich vystupu je mimo\n
  rozsah desky s adresou %d\n
  max pocet vystupu je %d\n
\t\n
Seznam kontrol:\n
1. Zmente konfiguraci pro tuto desku
1036:
Nazev mimo rozsah\n
Popis\Duvod:\n
- Pocet znaku v nazvu %s je vetsi\n
  nez %d znaku, nebo\n
  nazev chybi.\n
\t\n
Seznam kontrol:\n
1. Zadejte novy nazev, odpovidajici\n
   temto mezim.
1037:
Porucha propojeni V/V\n
Popis\Duvod:\n
- Signal %s existuje v OD i v DO\n
  ve stejnem retezu\n
\t\n
Seznam kontrol:\n
1. Opravte konfiguraci propojeni, kde je\n
   pripojen shora zmineny signal.
1038:
Propojeni V/V je moc hlub\n
Popis\Duvod:\n
- Propojeni ve stejnem retezu\n
  je prilis hluboko.\n
- Nazev prvniho signalu: %s\n
\t\n
Seznam kontrol:\n
1. Snizte hloubku propojeni.
1041:
Preteceni analog. vystupu\n
Popis\Duvod:\n
- Pocet analogovych vystupu pro\n
  desku %s je vetsi nez %d.\n
\t\n
Seznam kontrol:\n
1. Snizte pocet analogovych vystupu.
1042:
Preteceni analog. vstupu\n
Popis\Duvod:\n
- Pocet analogovych vstupu pro\n
  desku %s je vetsi nez %d.\n
\t\n
Seznam kontrol:\n
1. Snizte pocet analogovych vstupu.
1043:
Chyba typu signalu\n
Popis\Duvod:\n
- Typ specifikovany pro signal %s\n
  nelze ke specifikovane desce pripojit\n
\t\n
Seznam kontrol:\n
1. Zmenta na jiny typ.\n
2. Zmente na jinou desku.
1044:
Preteceni fyzick. signalu\n
Popis\Duvod:\n
- Rozah fyz. signalu, nebo delka, nebo\n
  fyz. signal a delka pro signal %s je\n
  vetsi nez %d\n
\t\n
Seznam kontrol:\n
1. Zmente cislo fyzickeho signalu.\n
2. Zmente delku.
1045:
Chyba specifikace filtru\n
Popis\Duvod:\n
- Signal %s : pro tento typ signalu\n
  nelze specifikovat zadny cas filtru.\n
\t\n
Seznam kontrol:\n
1. Nastavte cas filtru na 0\n
   nebo odstrante prikaz.
1046:
Chyba zmeny meritka\n
Popis\Duvod:\n
- Signal %s: nelze provadet zadnou\n
  zmenu meritka.\n
\t\n
Seznam kontrol:\n
1. Odstrante prikazy zmeny meritka.
1049:
Chyba inverse parametru\n
Popis\Duvod:\n
- Signal %s: tento typ signalu\n
  nelze invertovat.\n
\t\n
Seznam kontrol:\n
1. Invertovat lze pouze digitalni\n
   signaly.
1050:
Signal propoj neni digit\n
Popis\Duvod:\n
- Signal %s: neni digitalni signal\n
\t\n
Seznam kontrol:\n
1. Propojovat lze pouze digitalni\n
   signaly.
1052:
Krizova tabulka plna\n
Popis\Duvod:\n
- Celkovy pocet signalu OD secteny\n
  s celkovym poctem signalu DO\n
  nesmi prekrocit %d\n
\t\n
Seznam kontrol:\n
1. Snizte pocet signalu.\n
2. Zvyste pocet dovolenych propojeni.
1053:
Spojeni s desk. nefunguje\n
Popis\Duvod:\n
- Pristup k desce nelze zridit, protoze\n
  komunikace nefunguje\n
\t\n
Seznam kontrol:\n
1. Zkontrolujte komunikacni kabel\n
   k desce\n
2. Zkontrolujte, zda deska neni vypnuta
1054:
Chybny typ signalu\n
Popis\Duvod:\n
- Signal %s:\n
  Typ signalu je chybny\n
\t\n
Seznam kontrol:\n
1. Zmente typ
1055:
Neplatny nazev signalu\n
Popis\Duvod:\n
- Symbol %s: neni definovan\n
\t\n
Seznam kontrol:\n
1. Zmente nazev vyse uvedeneho symbolu
1056:
Obnov. poruch napaj. plne\n
Popis\Duvod:\n
- Symbol %s: nastaveni nebylo mozne\n
  pro obnovovani napajeni po vypadku.\n
  Tabulka poruch napajeni je plna.\n
\t\n
Seznam kontrol:\n
1. Zvetsete tabulku ve spoustecim\n
   souboru.\n
2. Ze seznamu obnoveni odstrante\n
   nektere signaly.
1058:
Zadny kontakt s uzlem Can\n
Popis\Duvod:\n
- Zadny kontakt s uzlem Can\n
  pripojenym k adrese uzlu %d\n
\t\n
Seznam kontrol:\n
1. Zkontrolujte adresy uzlu na vsech can\n
   modulech pripojenych ke sbernici can\n
2. Zmente adresu uzlu
1059:
Chyba konfig. uzlu Can\n
Popis\Duvod:\n
- Chyba pri konfiguraci uzlu Can\n
  pripojeneho k adrese uzlu %d\n
\t\n
Seznam kontrol:\n
1. Opravte konfiguraci pro\n
   uzel Can na dane adrese.
1061:
Chyba sbernice Can\n
Popis\Duvod:\n
- Abnormalni vyskyt chyb\n
  na sbernici Can pripojene k DSQC319\n
  na adrese %d\n
\t\n
Seznam kontrol:\n
1. Zkontrolujte komunikacni kabel\n
   ke sbernici Can
1072:
Zadne ulozeni pri signalu\n
Popis\Duvod:\n
- Signal %s\n
  nenastavil atribut Ulozit na ANO\n
\t\n
Seznam kontrol:\n
1. Nastavit atribut Ulozit.
1073:
Zrizen kont. s uzlem Can\n
Popis\Duvod:\n
- Kontakt zrizen s uzlem Can, pripojenym\n
  k adrese uzlu %d\n
\t\n
Seznam kontrol:\n
1. Neni treba nic delat.
1074:
Konfigurace mimo rozsah\n
Popis\Duvod:\n
- Pocatecni kvadrant IBS a velikost ramu\n
  jsou pro desku %s mimo rozsah\n
\t\n
Seznam kontrol:\n
1. Pro pocatecni kvadrant 1 musi byt\n
   velikost ramu mensi nez 5
1076:
Chyba komunikace od rtp1\n
Popis\Duvod:\n
- Tato seriova linka nema zadnou odezvu\n
\t\n
Seznam kontrol:\n
1. Zkontrolujte zarizeni nebo pripojeni
1077:
Chyba komunikace od rtp1\n
Popis\Duvod:\n
- Nelze dorucit prijatou zpravu\n
\t\n
Seznam kontrol:\n
1. Zkontrolujte komunikacni tok
1078:
Chyba komunikace od rtp1\n
Popis\Duvod:\n
- Odezva zarizeni ma sekvenci neplatneho\n
  zarizeni\n
\t\n
Seznam kontrol:\n
1. Zkontrolujte sum na seriove lince
1079:
Vystup pulsujici skupiny\n
Popis\Duvod:\n
- Vystup pulsujici skupiny neni dovolen.\n
\t\n
Seznam kontrol:\n
1. ---
1080:
Tabulka ovladace je plna.\n
Popis\Duvod:\n
- Pocet ovladacu nesmi prekrocit %d\n
\t\n
Seznam kontrol:\n
1. Omezte pocet ovladacu.\n
2. Zvyste pocet dovolenych ovladacu.
1081:
Fyzicka tabulka je plna.\n
Popis\Duvod:\n
- Pocet fyzickych signalu\n
  nesmi prekrocit %d\n
\t\n
Seznam kontrol:\n
1. Snizte pocet fyzickych signalu.\n
2. Zvyste pocet dovolenych fyz. signalu.
1082:
Tabulka signalu je plna.\n
Popis\Duvod:\n
- Pocet uzivatelem definovanych signalu\n
  nesmi prekrocit %d\n
\t\n
Seznam kontrol:\n
1. Snizte pocet signalu.\n
2. Zvyste pocet dovolenych signalu.
1083:
Tabulka symbolu je plna.\n
Popis\Duvod:\n
- Pocet symbolu\n
  nesmi prekrocit %d\n
\t\n
Seznam kontrol:\n
1. Snizte pocet symbolu.\n
2. Zvyste pocet dovolenych symbolu.
1084:
Tabulka spousteni plna\n
Popis\Duvod:\n
- Pocet ucastnickych signalu\n
  nesmi prekrocit %d\n
\t\n
Seznam kontrol:\n
1. Snizte pocet ucastnickych signalu.\n
2. Zvyste pocet dovolenych ucastnickych\n
   signalu.
1085:
Tabulka jednotek je plna.\n
Popis\Duvod:\n
- Pocet desek\n
  nesmi prekrocit %d\n
\t\n
Seznam kontrol:\n
1. Snizte pocet definovanych desek.\n
2. Zvyste pocet dovolenych desek.
1094:
Mnoho def. ucast. propoj.\n
Popis\Duvod:\n
- Propojeni ma prilis mnoho\n
  signalu "Od" : %s\n
\t\n
Seznam kontrol:\n
1. Zkontrolujte konfiguraci propojeni.
1095:
Dlouhy ret. ucast. propoj\n
Popis\Duvod:\n
- Cast "Od" v retezci ucastniku\n
  propojeni je prilis dlouha : %s\n
\t\n
Seznam kontrol:\n
1. Zkontrolujte konfiguraci propojeni.
1097:
Chyba ukladani parametru\n
Popis\Duvod:\n
- Signal %s: tento typ signalu\n
  nemuze mit moznost ulozeni.\n
\t\n
Seznam kontrol:\n
1. Moznost ulozeni maji jen digitalni\n
   signaly.
1098:
NFS server lost\n
Description\Reason:\n
The contact with the NFS server\n
'%s' is lost.\n
\t\n
Check:\n
1. The NFS server.\n
2. The network connection.\n
3. The controller configuration.
1099:
Trusted NFS server lost\n
Description\Reason:\n
The contact with the trusted\n
NFS server '%s'\n
is lost.\n
\t\n
Check:\n
1. The NFS server.\n
2. The network connection.\n
3. The controller configuration.
1101:
Unknown bus name.\n
Description\Reason:\n
- Board %s: Unknown bus\n
  name %s\n
\t\n
Check list:\n
1. Change the bus name for the board\n
   at unit type configuration.
1102:
DeviceNet incompatible\n
Description\Reason:\n
- Node %d:\n
  Internal info:\n
  %s,%d\n
  (%s)\n
\t\n
Check list:\n
1. Disconnect the node from bus\n
2. Contact ABB.
1103:
Error on I/O Bus\n
Description\Reason:\n
- An abnormal rate of errors on the\n
  %s Bus has been detected.\n
  The connector for Robot CAN I/O\n
  has been switched off\n
\t\n
Check list:\n
1. Check bus terminators.\n
2. Check I/O bus for short-circuit.\n
3. Restart system.
1104:
Error on I/O Bus\n
Description\Reason:\n
- An abnormal rate of errors on the\n
  %s Bus has been detected.\n
The connectors for External CAN I/O\n
and Robot CAN I/O has been switched off\n
\t\n
Check list:\n
1. Check bus terminators.\n
2. Check I/O bus for short-circuit.\n
3. Restart system.
1113:
IBS user command failure\n
Description\Reason:\n
- Warning due to: %d\n
\t\n
Check list:\n
1. Check the InterBus-S configuration\n
   according to above error code.
1114:
Invalid IP address\n
Description\Reason:\n
'%s' is not a valid IP address\n
\t\n
Check list:\n
1.Check the Communication configuration.
1115:
Invalid subnet mask\n
Description\Reason:\n
'%s' is not a valid subnet mask\n
\t\n
Check list:\n
1. Check the Communication configuration
1117:
Battery superv. res.\n
Description\Reason:\n
The battery capacity = %d\n
\t\n

1118:
Battery superv. state\n
Description\Reason:\n
The battery supervision is in wrong\n
state .\n
The state is = %s\n
\t\n

1119:
IO-unit table full.\n
Description\Reason:\n
- Maximum number of IO-units\n
  of type %s exceeded.\n
  Max = %d\n
\t\n
Check list:\n
1. Reduce the number of IO-units.
1120:
RAP option not installed\n
Description\Reason:\n
The RAP Communication option has to be\n
installed when configuring RAP or\n
using SCWrite.\n
\t\n
Check list:\n
1. Reboot and install the\n
   RAP Communication option.
1121:
RAP start-up failed\n
Description\Reason:\n
The initialization of RAP failed.\n
\t\n
Check list:\n
1. Check internal log for description.
1122:
Incorrect IP address\n
Description\Reason:\n
The address '%s'\n
in protocol '%s'\n
is not a correct IP address.\n
\t\n
Check list:\n
1. Change the address.
1123:
No transmission protocol\n
Description\Reason:\n
The transmission protocol '%s'\n
given for application protocol '%s'\n
could not be found.\n
\t\n
Check list:\n
1. Change the transmission protocol.
1124:
Wrong transmission prot.\n
Description\Reason:\n
The transmission protocol for\n
the NFS protocol '%s' must be\n
TCP/IP.\n
\t\n
Check list:\n
1. Change the transmission protocol.
1125:
Mount Permission denied\n
Description\Reason:\n
Permission was denied to mount\n
the directory '%s'\n
on the server '%s'.\n
\t\n
Check list:\n
1. Change the User or Group ID.
1126:
Directory not exported\n
Description\Reason:\n
Mounting directory '%s'\n
as '%s' failed\n
since it is not exported on the server\n
computer '%s',Protocol: '%s'.\n
\t\n
Check list:\n
1. Export the directory on\n
   the server computer.
1127:
ID's not the equal\n
The User and Group ID's has to have\n
the same value for all remote disks\n
\t\n

1128:
Ethernet not installed\n
Description\Reason:\n
The Ethernet Services option has to be\n
installed when using remote mounted\n
disk.\n
\t\n
Check list:\n
1. Reboot and install the Ethernet\n
   Services option.
1129:
Too many remote disks\n
Description\Reason:\n
The maximum number of remote mounted\n
disks is '%d'.\n
\t\n
Check list:\n
1. Reduce the number of remote mounted\n
   disks.
1130:
Too many remote servers\n
Description\Reason:\n
The maximum number of servers for\n
remote mounted disk is '%d'.\n
\t\n
Check list:\n
1. Reduce the number of servers.
1131:
Could not mount directory\n
Description\Reason:\n
Mounting directory '%s'\n
on the computer '%s' failed\n
Protocol: '%s'.\n
\t\n
Check list:\n
1. Check the server setup.
1132:
Battery superv. block\n
Description\Reason:\n
The battery superviosion is blocked\n
becaurse a power off/on is made.\n
Will be released %s\n
\t\n

1133:
Battery not charged\n
Description\Reason:\n
The battery is not charged after\n
the first charging state.\n
\t\n
Check list:\n
1. Check that the batlow signal is\n
   connected to the DSQC347.\n
2. Check the battery connections\n
3. Check the battery.
1137:
Error code from unit\n
Description\Reason:\n
-Error code from I/O unit: %s\n
The following error was returned:\n
%s\n
\t\n
Check list:\n
1. Check unit parameter configuration.
1139:
Access error from IO\n
Description\Reason:\n
- Cannot Read or Write signal %s\n
  due to communication down.\n
\t\n
Check list:\n
1. Check 'No contact with I/O unit'\n
   report for reason.
1140:
Parameter act high error\n
Description\Reason:\n
- Signal %s: This type of signal\n
  can't be set to active high.\n
\t\n
Check list:\n
1. Only output signals can be\n
   set to active high.
1141:
Default out of range\n
Description\Reason:\n
- The default value for\n
	signal %s is out of range\n
\t\n
Check list:\n
1.Change the default value in\n
  configuration.
1142:
Parameter Default error\n
Description\Reason:\n
- Signal %s: This type of signal\n
  can't be assigned a default value\n
\t\n
Check list:\n
1. Only output signals can be assigned\n
	default values.
1143:
CTS/RTS not allowed\n
Description\Reason:\n
- Serie channel %s:\n
  can't have option RTS/CTS.\n
\t\n
Check list:\n
1. Remove the option from configuration.
1146:
Subscribe error\n
Description\Reason:\n
- The maxlimit is less then minlimit\n
  maxlimit = %f minlimit = %f.\n
\t\n
Check list:\n
1. Make the correction and try again
1153:
Can't access parameter\n
Description\Reason:\n
- Unit %s has parameters\n
  that can't be edited from\n
  the teach pendant.\n
\t\n
Check list:\n
1. Save the EIO configuration to\n
   a file\n
2. Use a text editor to change\n
   the parameters
1156:
IPC queue full\n
Description\Reason:\n
- The ipc queue %s was\n
  full, when sending to trap routine.\n
\t\n
Check list:\n
1. Restart the system
1157:
Invalid app type\n
Description\Reason:\n
- Com Unit %s: has an unspecified\n
  Com app type named: %s.\n
\t\n
Check list:\n
1.Check the Com app type against\n
  the one specified for the Com app
1159:
Signal Access illegal\n
Description\Reason:\n
- Signal %s:\n
  The number of characters in\n
  Access %s\n
  is greater than %d or name missing.\n
\t\n
Check list:\n
1. Give a new Access that fits within\n
   the limits.
1160:
Access level illegal\n
Description\Reason:\n
- Signal %s:\n
  Access level %s in\n
  group %s is illegal.\n
- Legal choices all/man/auto/none.\n
\t\n
Check list:\n
1. Give a new access level for group\n
   that fits.
1161:
Access name not found\n
Description\Reason:\n
- Signal %s\n
  The Access name %s\n
  not found in EIO_USER_ACCESS.\n
\t\n
Check list:\n
1. Define %s in EIO_USER_ACCESS\n
   or change Access name.
1163:
Signal on internal unit\n
Description\Reason:\n
- Signal %s is not allowed\n
  to connect to %s\n
  because the unit is internal\n
\t\n
Check list:\n
1. Connect the signal to another unit
1164:
Internal signal in cross\n
Description\Reason:\n
- Signal %s is not allowed\n
  to be cross connected to\n
  signal %s\n
\t\n
Check list:\n
1. Make sure that none of the signals\n
   are internal.
1165:
FTP server went down\n
Description\Reason:\n
The connection to a non-trusted\n
FTP server has been lost.\n
\t\n
Check list:\n
1. Check cable and FTP server settings.
1166:
FTP server went down\n
Description\Reason:\n
The connection to a trusted\n
FTP server has been lost\n
\t\n
Check list:\n
1. Check cable and FTP server settings.
1167:
Wrong transmission prot.\n
Description\Reason:\n
Wrong transmission protocol\n
was found in the configuration\n
for protocol '%s'.\n
Only TCP/IP is supported.\n
\t\n
Check list:\n
1. Change the transmission protocol.
1168:
Could not login\n
Logon to FTP server was denied\n
because of unknown username and/or\n
password.\n
\t\n
Check list:\n
1. Check that username and passwords\n
are the same on FTP server and robot.
1169:
Ethernet not installed\n
Description\Reason:\n
The Ethernet option with FTP is not\n
installed on this system.\n
\t\n
Check list:\n
1. Reboot and install the Ethernet\n
   Services with FTP option.
1171:
Illegal I/O Unit\n
Description\Reason:\n
- The unit type %s used by unit\n
  %s is a non ABB device\n
\t\n
Check list:\n
1. Make sure that the I/O Plus Option\n
   is installed
1205:
Could not mount dir\n
Description\Reason:\n
Mounting directory '%s'\n
on the computer '%s' failed\n
Protocol: '%s'.\n
\t\n
Check list:\n
1. Check the FTP server setup
1231:
Wrong Profibus file\n
Description\Reason:\n
- Profibus binary file is not accepted\n
  by unit %.16s at address:\n
  %.4d.\n
  The unit can not be enabled.\n
\t\n
Check list:\n
1. Check the binary file\n
2. Check the unit type\n
3. Check the unit address
1262:
Fieldbus comm. failure\n
Description\Reason:\n
Communication with\n
'%s'\n
master failed on unit with mac id\n
'%d'\n
\t\n
Check list:\n
1. Check the connection to the gateway
1263:
CAN comm. failure\n
Description\Reason:\n
CAN communication failed due to\n
'%s'\n
code:'%d'\n
\t\n
Check list:
1278:
Mount Permission denied\n
Description\Reason:\n
Permission was denied to mount\n
the directory '%s'\n
on the server '%s'.\n
\t\n
Check list:\n
1. Check the username and password.
1288:
Mount Path too large\n
Description\Reason:\n
Mount path is too large. Mount path =\n
FTP server mount point + server path.\n
Max length: '%d'.\n
Protocol: '%s'.\n
\t\n
Check list:\n
1. Change FTP server mount point or\n
   server path.
1289:
Memory partition too big\n
Description\Reason:\n
The mem partition for communication\n
purposes cannot be allocated.\n
The requested partion = %d kB.\n
System memory partition will be used.\n
\t\n
Check list:\n
1. Decrease commPartSize.
1290:
Failed to add FTP device\n
Description\Reason:\n
Adding the FTP device '%s'\n
to the operating system failed.\n
Application protocol: %s.\n
\t\n
Check list:\n
1. Try to change local path.
1291:
Invalid local path\n
Description\Reason:\n
Local path for FTP device '%s'\n
is invalid.\n
\t\n
Check list:\n
1. Local path must end with ':'.
