###################################################################
#
# rlpider.eng  -  Calibration pendelum english error text description file  
#
# $Revision: 1.2 $
#
# DESCRIPTION:
#
#  ReaL error text description file
# 
# DEFINITION AND TRANSLATION RULES
# 
# (1) ERROR TEXT:
#     - String that will be a part of some error message from the system
#
#
# MODIFICATIONS:
#
#
# Copyright (c) ABB Robotics AB 2002  All rights reserved
#
############################################################################## 
#
#
CALPEND::
# Type of text object : ERROR TEXT 
# Explanation........ :
# Max. no of chars....: 40 
100:
Error reading from device

# Type of text object : ERROR TEXT 
# Explanation........ :
# Max. no of chars....: 40 
101:
Sensor A incorrectly connected

# Type of text object : ERROR TEXT 
# Explanation........ :
# Max. no of chars....: 40 
102:
Wrong address for sensor A

# Type of text object : ERROR TEXT 
# Explanation........ :
# Max. no of chars....: 40 
103:
Sensor B incorrectly connected

# Type of text object : ERROR TEXT 
# Explanation........ :
# Max. no of chars....: 40 
104:
Wrong address for sensor B

# Type of text object : ERROR TEXT 
# Explanation........ :
# Max. no of chars....: 40 
105:
No contact with Unit

# Type of text object : ERROR TEXT 
# Explanation........ :
# Max. no of chars....: 40 
106:
Unexpected error!

# Type of text object : ERROR TEXT 
# Explanation........ :
# Max. no of chars....: 40 
107:
Incorrect COM2 setup.
#        10        20  24    30        40
#--------|---------|---|-----|---------|	


# Note: calpender.eng starts at 100
#       calpendop.eng starts at 200
# End of file















