4::
0:

1:
Inputs/Outputs
2:
Invert:
3:
Groups
4:
Most Common
5:

6:

7:
Name:
8:
Value:
9:
Type:
10:

11:
Bus:
12:
Open
13:
Close
14:
Set
15:
Reset
16:
1
17:
0
18:
File
19:
Print...
20:
Preferences...
21:
Edit
22:
Alias Digital Out
23:
Alias Analog
24:
Goto...
25:
Goto Top
26:
Goto Bottom
27:
AliasIO
28:
View
29:
Most Common
30:
I/O units
31:
Digital In
32:
Digital Out
33:
Analog
34:
Alias Digital In
35:
Groups
36:
Alias All signals
37:
All signals
38:
Alias Groups
39:
Safety
40:

41:

42:

43:
Address:
44:
I/O unit:
45:
Signal:
46:

47:
Signal attributes:
48:
State
49:
I/O units
50:
OK
51:
Sigstate
52:
Cancel
53:
Result
54:
Incl
55:
Excl
56:
Goto Line!
57:
Enter Line
58:
Change
59:
Name              Value      Type
60:
Bus Addr Enabled Name        Type
61:
Name            Most Common  Type
62:
Name              Value      Signals
63:
No  Value    I/O Unit      Signal
64:
Group:
65:
Name              Value      Signal
66:
Up
67:
Move
68:
Setup
69:
Name                         Type
70:
Most Common Result
71:
Most Common Setup
72:
Off
73:
On
74:
False
75:
True
76:
Passive
77:
Active
78:
Low
79:
High
80:
Unit type:
81:

82:

83:
No signals
84:
Press Enter to proceed
85:
No signals mapped to unit
86:
Enter Value for IO Group
87:
Limits: Minimum
88:
        Maximum
89:
Data input for Inputs/Outputs
90:
Enter Value for Analog Signal
91:
Inputs/Outputs Printing
92:
Print
93:
Print Only to File :
94:
Add Signal Info    :
95:
Data to Print
96:
Print Inputs/Outputs to File:
97:
Printing !
98:
   To Cancel Press Enter
99:
 Press Enter to Continue
100:
Printer is Busy\n
\n
Try again when printer is ready
101:
Cannot Print because too many\n
print job queued\n
\n
Try again later
102:
Cannot Print because\n
Printer Device not configured\n
in System Parameters
103:
Not enough free space on unit\n
used when printing (usually\n
%.9s). Needs %d bytes\n
Please Move/Delete some files
104:
  Busy\n
\n
  Wait Please
105:
 Cannot create/write to file:\n
\n

106:
 File already exist\n

107:
Start Signal
108:
Cannot include signal!\n
The most common list may only\n
contain %d signals.
109:
Cannot change group value!\n
\n
The selected group contains\n
signals loaded as internal.
110:
Blocked
111:
Blocked:
112:
Yes
113:
No
114:
-
115:
Block
116:
Unblock
117:
Blocked
118:
Unblock all
119:
Some signals are blocked.\n
Unblock all signals?
120:
Enable Block function key
121:
Disable Block function key

122:
Signals       Value

123:
Special

124:
I/O Buses
125:
Bus
126:
Restart
127:
I/O buses
128:
Enable
129:
Disable
130:
Cannot enable unit!\n
\n
Possible causes:\n
   - Trustlevel restriction\n
   - Descriptor invalid
131:
Cannot disable unit!\n
\n
Possible causes:\n
   - Trustlevel restriction\n
   - Descriptor invalid
