54::

27:
write protected

28:
not valid for a digital write operation

29:
not valid for a analog write operation

30:
not valid for a digital read operation

31:
not valid for a analog read operation

42:
not valid for an alias operation

43:
Could not access the

44:
time event generator.

46:
Unable to read I/O signal.\n

47:
Unable to write I/O signal.\n

48:
Configuration error for I/O signal.\n

49:
Check the IO signals configuration\n
or alias definition.

50:
Unable to read the I/O signal\n
%s in unit %s.\n

51:
Unable to write to the I/O signal\n
%s in unit %s.\n

56:
The delay time has to be positive.\n

