RLDAP::
100:
The max string length of the parameter\n
%.16s is 5 characters.\n
See specification in %.16s
101:
Check the string data value
102:
The range of the parameter\n
%.16s is only valid\n
from 1 - 4.\n
See specification in %.16s
103:
Check the num data value
104:
The specified signal %.16s\n
in the instruction %.16s\n
has no reference
105:
Check the EIO configuration
106:
The optional signals \%.6s and\n
\%.6s must be used together.\n
See specification in %.16s
107:
Check the program
108:
The inparameter %.16s of\n
the instruction %.16s is\n
not an array
109:
Check the data definition
110:
The dimension of the data array\n
%.16s is to big. See\n
specification in %.16s
111:
Check the data declaration
112:
The array %.16s of the\n
instruction %.16s is not\n
right defined
113:
Check the data against the\n
specification
114:
The event time array element\n
%.16s%.3s is less than 0.\n
See spec. in %.16s
115:
Check the time event data
116:
The data selector %.16s in\n
the instruction %.16s\n
is not valid
117:
Check the selector against\n
the specification
118:
The selector %.16s in\n
the instruction %.16s\n
is not valid
119:
Check the selector against\n
the specification
120:
Missing optional argument in\n
instruction %.16s. It must\n
be spec. \%.8s or \%.6s
121:
See specification for this\n
instruction
