104::
0:
Pick & Place
1:
Item nr. eksisterer\n
Item nr. %.16s eksisterer\n
allerede. To item nr. må ikke\n
være ens.\n
%.40s\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

2:
Ikke et gyldig navn\n
Vælg %.16s\n
eller %.16s\n
eller %.16s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

3:
Buffer overskredet\n
Fatal intern fejl for item nr.\n
%.16s. Prøv varm - eller kold\n
start. Reporter denne fejl.\n
%.40s\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

4:
Item nr. ikke defineret\n
Item objekt er ikke blevet\n
defineret.\n
%.40s\n
%.40s\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

5:
Item nr. intern fejl\n
Intern fejl på item nr.\n
%.16s.\n
Fejl type: %.25s.\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

6:
Skyl item først\n
Item  %.16s skal skylles\n
før det bruges.\n
%.40s\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

7:
Ack. item mål først\n
Item mål skal kvitteres før\n
udførelse af GetItmTgt(s) instruktion\n
gentages. Item nr.: %.16s.\n
%.40s\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

8:
Item mål buffer fuld\n
Item mål buffer fyld med\n
item %.16s.\n
%.40s\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

9:
For mange item mål\n
For mange item mål er flyttet til\n
item %.16s.\n
%.40s\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

10:
Conveyer eio init. fejl\n
Fejl i installationen af\n
I/O signal for item nr.\n
%.16s, for conveyor\n
%.16s. Eio signal navn\n
%.16s.\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

11:
Conveyer eksisterer ikke\n
Fejl i item nr.\n
%.16s.\n
Cconveyer %.16s\n
eksisterer ikke.\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

12:
Conveyer navn ikke givet\n
Fejl i item nr.\n
%.16s.\n
Ingen conveyer navn specifiseret.\n
%.40s\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

13:
Conveyer grænse fejl\n
Fejl i item nr.\n
%.16s, conveyer\n
%.16s. Grænser er\n
ukorrekt specifiseret.\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

14:
Cnv data defineret sent\n
Fejl i item nr %.16s,conveyer\n
%.16s. ItmSrcCnvDat\n
instruktion skal kaldes før\n
ItmSrcFlush instruktion.\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

15:
Timeout\n
Instruktion har nået timeout\n
%.40s\n
%.40s\n
%.40s\n
\t\n
%.40s\n
\n
Genopretning: %.16s\n

16:
Sortdata overridden\n
Use of selection data will override\n
the sortdata.\n
%.40s\n
%.40s\n
\t\n
Item source: %.16s\n
Instruction:\n
%.40s\n
%.40s
17:
Orientation error\n
The orientation in selection data\n
is not correct defined.\n
\n
Item source: %.16s\n
%.16s %.16s\n
\t\n
All used orientations must be normal-\n
ized i.e. the sum of the quaternion\n
elements squares must equal 1.\n
Instruction:\n
%.40s
101:
Work object buffer fuld\n
For mange conveyer strobes gemt i\n
buffer for item nr. %.16s\n
In queue index: %16s\n
Out queue index: %16s\n
\t\n

102:
Item mål buffer fuld\n
Item mål buffer fyldt med\n
item nr. %.16s.\n
Item tag: %.16s.\n
Scene nummer %.16s.\n
\t\n

103:
For mange item mål\n
For mange item mål flyttet til\n
item nr. %.16s.\n
Antal af items: %.16s.\n
Scene number %.16s.\n
\t\n

104:
Push uden nogen strobe\n
Push modtaget uden korresponderende\n
strobe signal, modtaget for\n
item nr. %.16s.\n
\t\n
Push scene nummer %.16s\n
Senest modtaget strobe %.16s\n
\n
Check hardware forbindelser
105:
Push modtaget for sent\n
Push for items var modtaget for sent\n
i item nr. %.16s.\n
Korresponderende wobj overskrevet\n
\t\n
Push scene nummer %.16s\n
Senset modtaget strobe %.16s\n
\n
Check positions frekvens\n

106:
Conveyor limits error\n
Error in item source %.16s\n
Conveyor %.16s\n
The limits are incorrectly specified.\n
\t\n
Required: Enter < Exit\n
or: Enter < Start < Stop < Exit\n
Given: %.30s
107:
Trig distance warning\n
Trig distance is too long for\n
conveyor %.16s.\n
Trig distance is set to maximum.\n
Given:  %.30s\n
Max:  %.30s\n
\t\n

108:
Trig distance warning\n
Trig distance is too short for\n
conveyor %.16s.\n
Trig distance is set to minimum.\n
Given:  %.30s\n
Min:  %.30s\n
\t\n

109:
Failed to send data\n
An error occured when sending variable\n
%.16s from the item source\n
%.16s to remote system.\n
Status %.8s\n
\t\n
Check the position generation frequency\n
and the network connections.
110:
Failed to open signal\n
An error occured when opening\n
Position Generator signal:\n
%16s for item source:\n
%16s. Status %.8s\n
\t\n
Check the Position Generator\n
signal name.
111:
Failed to open signal\n
An error occured when opening\n
Trig signal: %16s\n
for item source: %16s.\n
Status %.8s\n
\t\n
Check the Trig signal name
112:
Failed to open signal\n
An error occured when opening\n
Strobe signal: %16s\n
for item source: %16s.\n
Status %.8s\n
\t\n
Check the Strobe signal name
113:
Failed to open signal\n
An error occured when opening\n
Robot Execution signal: %16s\n
for item source: %16s.\n
Status %.8s\n
\t\n
Check the Robot Execution signal name
114:
Failed to open signal\n
An error occured when opening\n
Queue Idle signal: %16s\n
for item source: %16s.\n
Status %.8s\n
\t\n
Check the Queue Idle signal name
115:
Failed to open signal\n
An error occured when opening\n
Position Available signal:\n
%16s\n
for item source: %16s.\n
Status %.8s\n
\t\n
Check the Position Available signal name
116:
Failed to open signal\n
An error occured when opening\n
Conveyor Control signal:\n
%16s\n
for item source: %16s.\n
Status %.8s\n
\t\n
Check the Conveyor Control signal name
