71::
0:
Arcweld
1:
Weld Tuning...
2:
Weave Tuning...
3:
(Seam Tuning)
4:
(Track Tuning)
5:
Blocking...
6:
Block
7:
Release
8:
Cancel
9:
OK
10:
AW Blocking
11:
To block a process, press Block
12:
To release a process, press Release
13:
Blocked
14:
Process
15:
x
16:

17:
Welding
18:
Weaving
19:
Tracking
20:
Weld
21:
Weave
22:
Track
23:
AW Weld Tuning
24:
Change Present value
25:
Welddata
26:
Tuning
27:
Present
28:
Select the data
29:
Origin >
30:
Pres >
31:
-
32:
+
33:
Revert
34:
AW Weave Tuning
35:
Weavedata
36:
Update
37:
Update origin value
38:
Origin
39:
Tuning   Present
40:
aw_inhibit
41:
weldBlocked
42:
weaveBlocked
43:
trackBlocked
44:
seamdata
45:
welddata
46:
weavedata
47:
Manual wirefeed...
48:
Gas on/off...
49:
AW Manual Wirefeed 
50:
To feed forward, press Fwd
51:
To feed backward, pres Bwd
52:
The wirefeed is going on as long as
53:
the function key is pressed.
54:
Fwd
55:
Bwd
56:
(Releas)
60:
bool
61:
Select AW system...
62:
System:
63:
Increments...
64:
AW Tuning increments
65:
Voltage:
66:
Distance:
67:
Wirefeed:
68:
Welding speed:
69:
Select AW system
70:
curr_aw_data
71:
curr_system_no
72:
curr_weld
73:
curr_weld_type
74:
curr_seam
75:
curr_seam_type
76:
curr_weave
77:
curr_weave_type
78:
string
80:
AW Manual Gas On/Off
81:
To activate, press Gas on
82:
The gas is on as long as
83:
The function key is pressed.
84:
Gas on
86:
                                       
87:
awproc_id
88:
ipm_id
89:
user_data
100:
AW Manual Sensor On/Off
101:
To activate sensor, press On
102:
To deactivate sensor, press Off
103:
On
104:
(On)
105:
Off
106:
(Off)
107:
Y:
108:
Z:
109:
Gap:
110:
*****
111:
Sensor coordinates
112:
Joint:   
113:
Sensor error\n
\n
   Communication error
114:
Sensor error\n
\n
   General error
115:
Sensor error\n
\n
   Sensor busy
116:
Sensor error\n
\n
   Unknown command
117:
Sensor error\n
\n
   Illegal variable number
118:
Sensor error\n
\n
   External alarm
119:
Sensor error\n
\n
   Camera error
120:
Sensor error\n
\n
   Temperature error
121:
Sensor error\n
\n
   Value out of range
122:
Sensor error\n
\n
   Camera check error
123:
OK   
124:
Sensor...
125:
(Sensor)
126:
Robot coordinates
127:
Calibration:   
140:
Meas. values...
141:
Measurement values
142:
         Present
143:
V
144:
A
145:
Voltage
146:
Current
147:
No data
148:

149:
Original value is zero.\n
Revert causes present value\n
to be zero.\n
\n
OK to revert?
150:
RotX:
151:
RotY:
152:
RotZ:

