################################################################################
# The text description file for Paint elog messages
# The English version
# A message is described according to:
# - line 1  	a header for the message log, Maximum 25 characters
# - line 2-x	The reason for message. Maximum 200 char (max 40 on each row) on 5 lines
# - line x+1	\t\n to separate reason from check list
# - line x+2-y	The check list for message. Maximum 200 char (max 40 on each row) on 5 lines
#
# $Revision: 1.17 $
#-------------------------------------------------------------------------------

############################################################
# File = pnt_elog.eng
# Text resource number = TX_RES_PNT_ELOG
95::

############################################################
# PURPOSE: Defines the name for the Category Paint.
#	   The name is used in the error dialog title 2
# LIMITS: no_of_char = 20  no_of_lines = 1
# USED: WINDOW_TITLE
#                  20
#-------------------|
0:
Paint

############################################################
# PURPOSE: Process and motion stopped
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1:
Equipment error\n
Paint process and motion stopped\n
\t\n
Check the paint equipment.

############################################################
# PURPOSE: Process stopped
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
2:
Equipment error\n
Paint process stopped\n
\t\n
Check the paint equipment.
############################################################
# PURPOSE: A trigplane missed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
3:
Trig plane error\n
In PaintL %s: One trig plane, %s,\n
is defined outside the programmed\n
path\n
\t\n
Change eventdata or reprogram path.
############################################################
# PURPOSE: Two trigplanes missed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
4:
Trig plane error\n
In PaintL %s: Two trig planes, %s\n
and %s, are defined outside the\n
programmed path.\n
\t\n
Change eventdata or reprogram path.
############################################################
# PURPOSE: Three trigplanes missed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
5:
Trig plane error\n
In PaintL %s: Three trig planes, %s,\n
%s, and %s, are defined outside the\n
programmed path.\n
\t\n
Change eventdata or reprogram path.
############################################################
# PURPOSE: Four trigplanes missed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
6:
Trig plane error\n
In PaintL %s: Four trig planes, %s,\n
%s, %s and %s, are defined outside the\n
programmed path\n
\t\n
Change eventdata or reprogram path.
############################################################
# PURPOSE: More than four trigplanes missed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
7:
Trig plane error\n
In PaintL %s: Four trig planes, %s,\n
%s, %s and %s and more are defined\n
outside the programmed path.\n
\t\n
Change eventdata or reprogram path.
############################################################
# PURPOSE: A SetBrush trigplane is missed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
8:
Trig plane error\n
In 'SetBrush n': One trig plane,\n
%s, is defined outside\n
the programmed path.\n
\t\n
Change eventdata or reprogram path.
############################################################
# PURPOSE: More than four  SetBrush trigplanes are missed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
9:
Trig plane error\n
More than four 'SetBrush' trig plane\n
events are defined outside the\n
programmed path\n
\t\n
Change eventdata or reprogram path.
############################################################
# PURPOSE: Conveyor position out of reach
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
10:
Conv pos out of reach\n
Programmed position for conveyor axis\n
has passed out of reach\n
Programmed conv pos: %s\n
Actual conv pos: %s\n
Note: Only first occasion is reported\n
\t\n
Reduce conveyor speed or modify\n
programmed robtarget(s).
############################################################
# PURPOSE: Trig counter error
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
11:
Trig counter error\n
Can't allocate trig counters\n
or there is no free counter\n
Trig error supervision disabled\n
\t\n
Reload program to enable\n
trig error supervision.
############################################################
# PURPOSE: Conveyor position out of reach
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
12:
ConveyorSync Off\n
ConveyorSync was turned off because\n
conveyor speed exceded lower limit\n
%s per cent\n
of nominal speed %s\n
\t\n
Check minimum sync speed in PaintWare\n
parameter.\n
Check conveyor speed setting.
############################################################
# PURPOSE: Conveyor position out of reach
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
13:
ConveyorSync On\n
ConveyorSync was turned on because\n
conveyor regain nominal speed\n
%s per cent\n
of nominal speed %s\n
\t\n
No action needed\n
The conveyor speed is Ok.
############################################################
# PURPOSE: 'Process ready' Timeout
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
14:
'Process ready' Timeout\n
'process ready input' not OK.\n
\t\n
Check equipment connected TO\n
'process ready input'\n
Increase 'Proc Ready timeout'
############################################################
# PURPOSE: Conveyor running
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
15:
Conveyor running\n
Signal 'c1NullSpeed' not OK\n
\t\n
Stop conveyor before proceeding\n
with program execution.
############################################################
# PURPOSE: Argument not an integer
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1000:
Argument error.\n
The argument is not an integer.\n
\t\n
Change the argument to an integer.
############################################################
# PURPOSE: Argument is not an array
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1001:
Argument error.\n
The argument is not an array.\n
\t\n
Change the argument to an array.
############################################################
# PURPOSE: Argument not a persistent variable
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1002:
Argument error.\n
The argument is not a persistent\n
variable.\n
\t\n
Change the argument to a persistent.
############################################################
# PURPOSE: The array argument has to many dimensions
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1003:
Argument error.\n
The array argument has too many\n
dimensions.\n
\t\n
Change the array to one dimension.
############################################################
# PURPOSE: The chosen brush table is not allowed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1004:
Brush table error.\n
Only brush table %s is allowed.\n
\t\n
Change to allowed brush table.
############################################################
# PURPOSE: The chosen brush number is not allowed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1005:
Brush number error.\n
Only brush numbers less than or\n
equal to %s is allowed.\n
\t\n
Change to allowed brush number.
############################################################
# PURPOSE: The chosen argument value is not allowed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1006:
Argument value error\n
Negative value for argument no. %s .\n
\t\n
Change argument value to\n
a positive number.
############################################################
# PURPOSE: The chosen signal argument did not exist.
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1007:
Non-existing output\n
Signal in arg. %s did not exist.\n
\t\n
Check signal definitions.\n
Define signal or find an existing signal
############################################################
# PURPOSE: The argument is outside applicator limits
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1008:
Applicator number error\n
Applicator number is greater than\n
number of applicators installed.\n
\t\n
'App' argument (if present) must\n
be in range from 1 to\n
'Number of apps'
############################################################
# PURPOSE: The chosen argument value is not allowed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1009:
Brushfactor too high\n
\t\n
Change brushfactor to a number between\n
1 and 500.

############################################################
# PURPOSE: The chosen argument value is not allowed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1010:
Brushtable does not exist\n
The following brushtable does not\n
exist: '%s'\n
\t\n
Brushtable must be a persistent array\n
of datatype brushdata.
############################################################
# PURPOSE: The chosen argument value is not allowed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1011:
Brushtable not an array\n
The following brushtable is not an\n
array: '%s'\n
\t\n
Brushtable must be a persistent array\n
of datatype brushdata.
############################################################
# PURPOSE: The chosen argument value is not allowed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1012:
Wrong datatype for table\n
The following brushtable is not of\n
datatype brushdata:\n
'%s'\n
\t\n
Brushtable must be a persistent array\n
of datatype brushdata.
############################################################
# PURPOSE: The chosen signal argument did not exist.
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1013:
Non-existing signal\n
The following signal did not exist:\n
'%s'\n
\t\n
Check signal definitions.\n
Define signal or find an existing signal
############################################################
# PURPOSE: The chosen signal argument did not exist.
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
1014:
Channel not installed\n
The factor no. specified in arg %s is\n
greater than the number of installed\n
channels\n
\t\n
Check installed options:\n
Gun control : Factor no range = <1>\n
3 ch. system: Factor no range = <1-3>\n
4 ch. system: Factor no range = <1-4>
############################################################
# PURPOSE: The argument is outside brushtable limits
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
2000:
Brush number error.\n
The brush number is outside the limits\n
for the activated brush table.\n
\t\n
Change argument within limits.
############################################################
# PURPOSE: There is no brushtable activated
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
2001:
Brush table error.\n
There is no brush table activated.\n
\t\n
Activate a brush table.

############################################################
# PURPOSE: Brush not activated
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
2002:
Brush not activated.\n
Brush outputs blocked because IpsEnable\n
for Applicator %s was not active.\n
\t\n
Activate IpsEnable output for this\n
Applicator.

############################################################
# PURPOSE: Emy or GM stop active
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
2003:
Equipment Enable rejected\n
Equipment could not be enabled due\n
to the following active stop signals:\n
%s\n
\t\n
Check Emy stop buttons, General mode\n
stop input and Cabin Interlock input.\n
Press Emy stop reset

############################################################
# PURPOSE: The symbol for named output not found
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
2500:
Unable to open symbol.\n
Output for symbol %s not found.\n
NOTE: No paint-related outputs available\n
      due to this error.\n
\t\n
1. Output for symbol not defined.\n
2. Output for symbol has wrong name.\n
3. Internal problem (memory etc..)\n
   Try a restart.

############################################################
# PURPOSE: PaintWare is not available/has not been installed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
2501:
Paint System not inst.\n
Paint System not available\n
or not installed.\n
\t\n
PaintWare process not activated, due to\n
incomplete Paint System configuration.\n
1. Use IPS option diskette to install.\n
2. Custom-configure Paint System\n
using the Teach Pendant.

############################################################
# PURPOSE: PaintWare is not available/has not been installed
# LIMITS: no_of_char = 25+40+40  no_of_lines = 1+5+5
# USED: ERROR_MESSAGE
#                       25             40
#------------------------|--------------|
2502:
NonEx plug on AEXB\n
The system is installed as an Ex-proof\n
system but there is a NonEx plug on\n
AEXB board.\n
\t\n
Replace the NonEx plug with\n
a certified Ex-proof plug.
#
#End of file

