88::
36:
The %s instruction can't be\n
executed while the system is\n
in a stop state
37:
The object that the\n
instruction %s,\n
was waiting for has been\n
dropped
38:
Rerun the instruction
39:
The instruction %s, was\n
interrupted, reason unknown
40:
User frame error\n
Not possible to get the coordinated\n
user frame
41:
No single number defined
42:
Axes error\n
The single axis is not init correctly
43:
Another %s instruction is\n
waiting for the object
44:
Another %s instruction is\n
waiting for a distance to\n
the object
45:
The %s instruction has\n
lost contact with the\n
conveyor.
46:
 mech unit is not a single
47:
The sensor process is not\n
init correctly
48:
The sensor is not activated
49:
The conveyor is not activated
50:
The %s instruction is already connected
51:
The parameter %s is negative
52:
Set it positive or to zero
53:
The parameter %s forces the\n
robot out of workspace
54:
Decrease the value
