
95::
0:
Lakovani
1:
Chyba zarizeni\n
Zastaveni lakovani a pohybu.\n
\t\n
Zkontrolujte lakovaci zarizeni.
2:
Chyba zarizeni\n
Zastaveni lakovani.\n
\t\n
Zkontrolujte lakovaci zarizeni.
3:
Trig plane error\n
In PaintL %s: One trig plane, %s,\n
are defined outside the programmed\n
path.\n
\t\n
Change eventdata or reprogram path.
4:
Trig plane error\n
In PaintL %s: Two trig planes, %s\n
and %s, are defined outside the\n
programmed path.\n
\t\n
Change eventdata or reprogram path.
5:
Trig plane error\n
In PaintL %s: Three trig planes, %s,\n
%s, and %s, are defined outside the\n
programmed path.\n
\t\n
Change eventdata or reprogram path.
6:
Trig plane error\n
In PaintL %s: Four trig planes, %s,\n
%s, %s and %s, are defined outside the\n
programmed path.\n
\t\n
Change eventdata or reprogram path.
7:
Trig plane error\n
In PaintL %s: Four trig planes, %s,\n
%s, %s and %s and more are defined\n
outside the programmed path.\n
\t\n
Change eventdata or reprogram path.
8:
Trig plane error\n
In 'SetBrush n': One trig plane,\n
%s, is defined outside\n
the programmed path.\n
\t\n
Change eventdata or reprogram path.
9:
Trig plane error\n
More than four 'SetBrush' trig plane\n
events are defined outside the\n
programmed path\n
\t\n
Change eventdata or reprogram path.
10:
Conv pos out of reach\n
Programmed position for conveyor axis\n
has passed out of reach\n
Programmed conv pos: %s\n
Actual conv pos: %s\n
Note: Only first occasion is reported\n
\t\n
Reduce conveyor speed or modify\n
programmed robtarget(s).
11:
Trig counter error\n
Can't allocate trig counters\n
or there is no free counter\n
Trig error supervision disabled\n
\t\n
Reload program to enable\n
trig error supervision.
12:
ConveyorSync Off\n
ConveyorSync was turned off because\n
conveyor speed exceded lower limit\n
%s per cent\n
of nominal speed %s\n
\t\n
Check minimum sync speed in PaintWare\n
parameter.\n
Check conveyor speed setting.
13:
ConveyorSync On\n
ConveyorSync was turned on because\n
conveyor regain nominal speed\n
%s per cent\n
of nominal speed %s\n
\t\n
No action needed\n
The conveyor speed is Ok.
14:
'Process ready' Timeout\n
'process ready input' not OK.\n
\t\n
Check equipment connected TO\n
'process ready input'\n
Increase 'Proc Ready timeout'
15:
Conveyor running\n
Signal 'c1NullSpeed' not OK\n
\t\n
Stop conveyor before proceeding\n
with program execution.
1000:
Chyba argumentu.\n
Argument neni typ integer.\n
\t\n
Zmente typ argunmentu na integer.
1001:
Argument error.\n
The argument is not an array.\n
\t\n
Change the argument to an array.
1002:
Chyba argumentu.\n
Argument neni persistentni\n
promenna.\n
\t\n
Zmente argument na persistentni.
1003:
Argument error.\n
The array argument has too many\n
dimensions.\n
\t\n
Change the array to one dimension.
1004:
Brush table error.\n
Only brush table %s is allowed.\n
\t\n
Change to allowed brush table.
1005:
Brush number error.\n
Only brush numbers less than or\n
equal to %s is allowed.\n
\t\n
Change to allowed brush number.
1006:
Argument value error\n
Negative value for argument no. %s .\n
\t\n
Change argument value to\n
a positive number.
1007:
Non-existing output\n
Signal in arg. %s did not exist.\n
\t\n
Check signal definitions.\n
Define signal or find an existing signal
1008:
Applicator number error\n
Applicator number is greater than\n
number of applicators installed.\n
\t\n
'App' argument (if present) must\n
be in range from 1 to\n
'Number of apps'
1009:
Brushfactor too high\n
\n
\t\n
Change brushfactor to a number between\n
1 and 500.
1010:
Brushtable does not exist\n
The following brushtable does not\n
exist: '%s'\n
\t\n
Brushtable must be a persistent array\n
of datatype brushdata.
1011:
Brushtable not an array\n
The following brushtable is not an\n
array: '%s'\n
\t\n
Brushtable must be a persistent array\n
of datatype brushdata.
1012:
Wrong datatype for table\n
The following brushtable is not of\n
datatype brushdata:\n
'%s'\n
\t\n
Brushtable must be a persistent array\n
of datatype brushdata.
1013:
Non-existing signal\n
The following signal did not exist:\n
'%s'\n
\t\n
Check signal definitions.\n
Define signal or find an existing signal
1014:
Channel not installed\n
The factor no. specified in arg %s is\n
greater than the number of installed\n
channels\n
\t\n
Check installed options:\n
Gun control : Factor no range = <1>\n
3 ch. system: Factor no range = <1-3>\n
4 ch. system: Factor no range = <1-4>
2000:
Brush number error.\n
The brush number is outside the limits\n
for the activated brush table.\n
\t\n
Change argument within limits.
2001:
Brush table error.\n
There are no brush table activated.\n
\t\n
Activate a brush table.
2002:
Brush not activated.\n
Brush outputs blocked because IpsEnable\n
for Applicator %s was not active.\n
\t\n
Activate IpsEnable output for this\n
Applicator.
2003:
Equipment Enable rejected\n
Equipment could not be enabled due\n
to the following active stop signals:\n
%s\n
\t\n
Check Emy stop buttons, General mode\n
stop input and Cabin Interlock input.\n
Press Emy stop reset
2500:
Unable to open symbol.\n
Output for symbol %s not found.\n
NOTE: No paint-related outputs available\n
      due to this error.\n
\t\n
1. Output for symbol not defined.\n
2. Output for symbol has wrong name.\n
3. Internal problem (memory etc..)\n
   Try a restart.
2501:
Paint System not inst.\n
Paint System not available\n
or not installed.\n
\t\n
PaintWare process not activated, due to\n
incomplete Paint System configuration.\n
1. Use IPS option diskette to install.\n
2. Custom-configure Paint System\n
using the Teach Pendant.
2502:
NonEx plug on AEXB\n
The system is installed as an Ex-proof\n
system but there is a NonEx plug on\n
AEXB board.\n
\t\n
Replace the NonEx plug with\n
a certified Ex-proof plug.
