17::
0:
IO Signals
1:
User Signals
2:
System 
3:
Groups
4:
Signal Name
5:
Unit Name
6:
Signal Type
7:
Signal Number
8:
Start Signal
9:
Group Length
10:
DI
11:
DO
12:
Safety 
13:
Unit Name
14:
Unit Type
15:
Unit Bus
16:
Digital Inputs
17:
Digital Outputs
18:
IO Boards
19:
Name        Unit        Type        Sig               
20:
Name        Unit        Len        Phsig
21:
Unit type
22:
Name        Type        Bus      Address
23:
GI
24:
GO
25:
System Inputs
26:
System Outputs
27:
Name
28:
Action
29:
Status
30:
MotorOn
31:
MotorOff
32:
CycleOn
33:
MotorOn
34:
MotorOff
35:
Start
36:
StartMain
37:
Stop
38:
StopCycle
39:
Interrupt
40:
LoadStart
41:
Argument
42:
Name        Action
43:
Name        Status
44:
-
45:
To
46:
From
47:
Cross connections
48:
From        To
49:
Analog Inputs
50:
Analog Outputs
51:
Address
52:
AO
53:
AI
54:
ResetEstop
55:
EmStop
56:
AutoOn
57:
RunchOk
58:
TCPSpeed
59:
Logical Max
60:
Physical Max
61:
Logical Min
62:
Physical Min
63:
Filter Passive
64:
Filter Active
65:
Inverted
67:
YES
68:
NO
69:
RIO Addr(octal)
70:
RIO Baud Rate
71:
RIO Start Group
72:
RIO Rack size
73:
RIO Last rack
74:
57.6 kB
75:
115 kB
76:
230 kB
77:
0
78:
2
79:
4
80:
6
81:
1/4
82:
1/2
83:
3/4
84:
FULL
85:
Error
86:
SyncExtAx
87:
BAS
88:
VME
89:
SIM
90:
ResetError
91:
CAN
92:
Slot Addr
93:
Store
94:
MotOnState
95:
MotOffState
96:
PFError
97:
MotOnStart
98:
StopInstr
99:
SysReset
100:
IBS Rack size
