55::

46:
Cannot open

47:
RAISE CODE:

48:
File or serial channel is not opened.

49:
File or serial channel is not\n
opened in a character-based mode

50:
File or serial channel is not\n
opened in a binary mode

51:
Could not access the file

52:
The parameter %.16s in

53:
is not an array.

54:
The output buffer must be specified\n
as an array of num

55:
is specified as a negative value.

56:
The parameter must be set positive.

57:
Could not access the

58:
time event generator.

59:
signal event generator.

60:
A timeout interrupt the execution of

61:
A digital input interrupt execution of

65:
Received data not numeric type

68:
Too many pending read requests

76:
The buffer element %i in

77:
is outside 0-255.

78:
All elements in the buffer\n
must have the value 0-255

80:
is outside the array.

88:
Not open or not a serial channel

89:
has improper data type

90:
non-value and semi-value types\n
may not be used

91:
not closed

95:
File or serial channel is not\n
opened for reading

96:
File or serial channel is not\n
opened for writing

98:
Expected type differs from read type in

99:
One or more bytes is not read properly.\n
The value of the read data might be\n
inconsistent


