5::

0:
Jogging

1:
Align...

2:
The alignment is started by moving the\n
joystick.

3:
Motion Supervision...

4:
The tool will be aligned along a\n
coordinate axis of "World".

5:
Turn Motion Supervision ON/OFF\n
Note: Only applies to jogging

6:

7:
Unit:

8:
Motion:

9:
Group:

10:
Coord:

11:
Tool:

12:
WObj:

13:
Incremental:

14:
Select desired data in the list:

15:
Jogging

16:
Robot Pos:     

17:

18:

19:
Linear

20:
Reorient

21:
Axes

22:
x y z

23:

Motor
24:
World

25:
Base

26:
Tool

27:
WObj

28:

29:

30:

31:

32:

33:

34:
2 1 3

35:
5 4 6

36:
4 5 6

37:
Position:  

38:
External:      

39:
Small

40:
Medium

41:
Large

42:
World

43:
Base

44:
Tool

45:
WObj

46:
1 2 3

47:
No

48:
Small

49:
Medium

50:
Large

51:
1

52:
2

53:
Jogging cannot be\n
used when a program\n
is executing.

54:
Jogging cannot be\n
used in automatic\n
mode.

55:
New

56:
Change

57:
Define

58:
User

59:
User

60:
Motion type

61:
Increments...

62:
User defined increments

63:
Change the values of the variable jog\n
increments used for the different\n
motion types.

64:
Linear:

65:
Robot axes:

66:
Reorientation:

67:
External axes:

68:
Value

69:
Same as medium incr.

70:
Limits

71:
mm

72:
deg

73:
Joystick lock:

74:
None

75:
None

76:
Motion Supervision State:

77:
ON

78:
OFF


79:
AbsAcc On 

80:
Payload:

81:
load

82:
Preferences...

83:
Alternatives:

84:
Add

85:
Remove

86:
Default

87:
Customize the jogging window

88:
Deactivate...

89:
Deact

90:
Deactivate mechanical unit.

91:
To deactivate, select mechanical unit\n
and press Deact.

92:
No valid mechanical units are available.

93:
(Deact)
94:
Selection not valid.\n
The work object is moved by\n
a mechanical unit that\n
currently is deactivated.\n
\n
Press ENTER to proceed.

