###################################################################
#
# rltool.eng  -  Class rltool real packet RAPID english text description file  
#
# $Revision: 1.2 $
#
# DESCRIPTION:
#
#  ReaL text description file
# 
# DEFINITION AND TRANSLATION RULES
# 
# This file refer to following type of top object in the RAPID
# Reference Manual: INSTRUCTION, FUNCTION or DATA TYPE
#
# Following general rules for ARL Identifiers must applies for translation to
# native language of all text objects:
# - Maximum general length of text object 16 characters
# - Characters means letters, digits or underscore _ (According ISO 8859-1)
# - The first character in an text object must be a letter
# - All characters are significant
# - Text object differing only in the use of corresponding upper and lower
#   case letters are considered the same
#
# Type of text objects to translate:
# (1) Name of INSTRUCTION:
#     - Max. 9 characters (Instruction Plock List) 
#     - Upper case letter for the first letter in one word. The rest of the word
#       in lower case letters. Normal abbreviation of several words.
#     - E.g. MoveL for Move Linear
# (2) Name of FUNCTION:
#     - Max. 9 characters. (Instruction Plock List)
#       Need for shorter for expression context.
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters. Normal abbreviation of several words.
#     - E.g. ReadNum for Read Numerical
# 
# (3) Name of REQUIRED PARAMETER:
#     - Must not be short (not in the program list)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. Speed
#
# (4) Name of OPTION PARAMETER:
#     - Must be short (in the program list)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. WObj for Work Object
#
# (5) Name of SWITCH PARAMETER:
#     - Must be short (in the program list)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. Conc for Concurrent
#
# (6) Name of DATA TYPE:
#     - Must not be short (not in the visible program list)
#     - Only lower case letters
#     - E.g. robtarget for robot target
#
# (7) Name of DATA COMPONENT:
#     - Must be short (in the program list)
#     - Only lower case letters
#     - E.g. robconf for robot configuration
#
# MODIFICATIONS:
#
# $Log: rltool.eng,v $
# Revision 1.2  1999/07/15 07:49:07  bjfu
# Patch: daki0207H09M30S46 Solved SPR: XX Test status: Comp Log: RW4.0/1
#
# Revision 1.2  1998/11/12 08:56:54  daki
# Removed GetIODesc
#
# Revision 1.1  1998/09/14  10:59:20  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.4  1998/09/12  17:45:46  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol
#
# Revision 1.1  1998/05/06  16:10:37  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.3  1998/05/06  14:41:14  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol
#
# Revision 1.3  1997/09/17  15:10:19  funadmin
# RFAC development of DataLog
#
# Revision 1.3  1997/09/16  08:54:00  frle
# FRFAC DataLog development
#
# Revision 1.2  1997/05/28  11:53:36  hery
# Hidden instruction GetIODesc added.
#
# Revision 1.1  1996/11/27  09:43:02  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.2  1996/11/27  09:06:55  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/project2/foxfun/rol/classlib/rltool
#
# Revision 1.1  1996/09/05  12:42:38  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.1  1996/09/05  12:40:58  roladmin
# Initial revision
#
# Revision 1.2  1996/08/30  07:54:48  sejo
# Update for introduction of rltooler.eng
#
# Revision 1.1  1996/08/30  06:34:09  sejo
# Initial revision
#
# Revision 1.1  1996/07/26  08:07:26  mibe
# Initial revision
#
#
#
############################################################################## 
#
# Text resource number = 93 this has to be allocated at tx.
93::
# Reference to system internal ReaL-class (do not translate)
0:
rltool
# Type of top object  : To a already installed type
# Ref. to top object  : 
# Type of text object : type 
# Full name.......... : num
# Note............... :
1:
num

# Type of top object  : To a already installed type
# Ref. to top object  : 
# Type of text object : type 
# Full name.......... : bool
# Note............... :
2:
bool

# Type of top object  : To a already installed type
# Ref. to top object  : 
# Type of text object : type 
# Full name.......... : string
# Note............... :
3:
string

# Type of top object  : To a already installed type
# Ref. to top object  :
# Type of text object : DATA TYPE
# Full name.......... : switch
# Note............... : 
4:
switch

# Type of top object  : To a already installed type
# Ref. to top object  :
# Type of text object : DATA TYPE
# Full name.......... : mecunit
# Note............... :
5:
mecunit

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : REQUIRED PARAMETER
# Full name.......... : Channel
# Note............... :
6:
Channel

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : REQUIRED PARAMETER
# Full name.......... : TestPoint
# Note............... :
7:
TestPoint

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : REQUIRED PARAMETER
# Full name.......... : OptData
# Note............... :
8:
OptData

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : Probe define
# Note............... :
9:
ProbeDefine

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : Probe reset
# Note............... :
10:
ProbeReset

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : REQUIRED PARAMETER
# Full name.......... : File
# Note............... :
11:
File

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : Probe save
# Note............... :
12:
ProbeSave


# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : Probe start
# Note............... :
13:
ProbeStart


# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : Probe stop
# Note............... :
14:
ProbeStop

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : Spy start
# Note............... :
15:
SpyStart

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : Spy stop
# Note............... :
16:
SpyStop

# INTERNAL SYSTEM USE
# DO NOT TRANSLATE OR CHANGE ANYTHING FOR TEXT NO 17
17:
ANYTYPE#

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : REQUIRED PARAMETER
# Full name.......... : Signal
# Note............... :
18:
Signal

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : DataLog reset
# Note............... :
20:
DataLogReset

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : REQUIRED PARAMETER
# Full name.......... : MechUnit
# Note............... :
21:
MechUnit

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : REQUIRED PARAMETER
# Full name.......... : Axis
# Note............... :
22:
Axis

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : OPTIONNAL PARAMETER
# Full name.......... : Scale
# Note............... :
23:
Scale

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : OPTIONNAL PARAMETER
# Full name.......... : Sample
# Note............... :
24:
Sample

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : DataLog define
# Note............... :
25:
DataLogDefine

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : REQUIRED PARAMETER
# Full name.......... : LogTime
# Note............... :
26:
LogTime

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : DataLog start
# Note............... :
27:
DataLogStart

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : REQUIRED PARAMETER
# Full name.......... : PreLogTime
# Note............... :
28:
PreLogTime

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : DataLog trigg
# Note............... :
29:
DataLogTrigg

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : OPTIONNAL PARAMETER
# Full name.......... : NoML
# Note............... :
30:
NoML

# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : DataLog save
# Note............... :
31:
DataLogSave

# End of file
