###################################################################
#
# rlraps.eng  -  Class rlraps english RAPID text description file  
#
# $Revision: 1.10 $
#
# DESCRIPTION:
#
#  ReaL text description file
# 
# DEFINITION AND TRANSLATION RULES
# 
# This file refer to following type of top object in the RAPID (ARL)
# Reference Manual: INSTRUCTION, FUNCTION or DATA TYPE
#
# Following general rules for ARL Identifiers must applies for translation to
# native language of all text objects:
# - Maximum general length of text object 16 characters
# - Characters means letters, digits or underscore _ (According ISO 8859-1)
# - The first character in an text object must be a letter
# - All characters are significant
# - Text object differing only in the use of corresponding upper and lower
#   case letters are considered the same
#
# Type of text objects to translate:
# (1) Name of INSTRUCTION:
#     - Max. 10 characters (Instruction Plock List) 
#     - Upper case letter for the first letter in one word. The rest of the word
#       in lower case letters. Normal abbreviation of several words.
#     - E.g. MoveL for Move Linear
# (2) Name of FUNCTION:
#     - Max. 10 characters. (Instruction Plock List)
#       Need for shorter for expression context.
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters. Normal abbreviation of several words.
#     - E.g. ReadNum for Read Numerical
# 
# (3) Name of REQUIRED PARAMETER:
#     - Max. 12 characters (Instruction Form)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. Speed
#
# (4) Name of OPTION PARAMETER:
#     - Must be short (in the program list)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. WObj for Work Object
#
# (5) Name of SWITCH PARAMETER:
#     - Must be short (in the program list)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. Conc for Concurrent
#
# (6) Name of DATA TYPE:
#     - Can be fairly long (not in the visible program list)
#     - Only lower case letters
#     - E.g. robtarget for robot target
#
# (7) Name of DATA COMPONENT:
#     - Must be short (in the program list)
#     - Only lower case letters
#     - E.g. robconf for robot configuration
#
# MODIFICATIONS:
#
# $Log: rlraps.eng,v $
# Revision 1.10  2004/05/19 17:00:23  SIGADMIN
# Patch: tofa1905H14M06S55 Solved SPR: 1017302 Test status: CL Log: New RAPID function NonMotionExecutionMode added;
#
# Revision 1.12  2004/05/19 12:06:16  tofa
# SPR 1017302
# Checked by: svjo
# New function nonexcecutionmode added
#
# Revision 1.11  2004-01-07 16:37:44+01  haugkjet
# SPR1016064 - New function GetSysInfo()
#
# Revision 1.10  2003-12-22 13:29:05+01  hajn
# SPR1016118
# Checked by SEJO
# New RAPID function FUNC num ProgMemFree()
#
# Revision 1.9  2001-11-20 13:49:09+01  hesve
# new text added for function cspeedoverride
#
# Revision 1.8  2001-02-15 12:57:26+01  hesve
# new text added for function gettaskname
#
# Revision 1.7  2000-10-17 12:45:08+02  sejo
# SPR-1007436 TextTabFreeToUse and TextTabInstall
#
# Revision 1.6  2000-10-11 14:16:00+02  sejo
# Add new function WarmStart
#
# Revision 1.5  2000-09-11 10:35:05+02  pihi
# New funciton, RobOS
#
# Revision 1.4  2000-06-15 16:50:16+02  sejo
# Partly development of MailSend
#
# Revision 1.3  1999-02-25 17:50:41+01  sejo
# Extended TriggStopProc with trigcounter and interrupt control
#
# Revision 1.2  1999/02/23  13:15:44  sejo
# New instruction TriggStopProc
#
# Revision 1.1  1998/09/14  10:52:29  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.7  1998/09/12  17:22:15  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol
#
# Revision 1.1  1998/05/06  16:04:01  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.6  1998/05/06  11:36:05  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol
#
# Revision 1.5  1997/12/09  09:25:57  sejo
# Add secret RAPID routines for LoadId
#
# Revision 1.4  1997/05/23  11:32:14  sejo
# SPR-1000518 RunMode with \Main
#
# Revision 1.3  1997/05/21  11:16:54  krha
# SingAreaWrist function
#
# Revision 1.2  1996/12/23  09:39:53  inre
# add skipwarn
#
# Revision 1.1  1996/11/27  09:38:41  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.5  1996/11/27  08:57:41  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/project2/foxfun/rol/classlib/rlraps
#
# Revision 1.6  1996/10/10  08:43:04  krha
# IsOptId and IsSysId functions added
#
# Revision 1.5  1996/09/02  07:33:07  anma
# Added new RAPID text items for new RAPID function BookErrNo.
#
# Revision 1.4  1996/08/27  14:35:40  krha
# Comments changed
#
# Revision 1.3  1996/08/27  14:14:15  anma
# Added the ARL function TextTabGet and his argument TableName.
#
# Revision 1.2  1996/04/11  14:08:34  anma
# Do somethings for advanced testing for textget.
#
# Revision 1.1  1996/04/09  13:51:32  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.4  1996/04/09  13:31:28  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/project2/foxfun/rol/classlib/rlraps
#
# Revision 1.2  1996/04/02  12:00:15  anma
# Add ArgName and TextGet
#
# Revision 1.1  1995/12/06  13:07:06  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.3  1995/12/06  12:36:58  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/project2/foxfun/rol/classlib/rlraps
#
# Revision 1.1  1995/04/12  11:57:01  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.2  1995/04/12  10:24:10  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib/rlraps
#
# Revision 1.3  1995/04/03  13:59:06  habr
# Addition of PFDOval, PFGOVal, PFRestart,
# PFIOResto.
#
# Revision 1.2  1994/08/16  09:29:01  sejo
# Max. instruction/function length 9 -> 10 characters
#
# Revision 1.1  1994/07/07  15:49:44  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.1  1994/07/07  10:27:11  roladmin
# Initial revision
#
# Revision 1.2  1994/06/16  08:57:54  habr
# no entry
#
# Revision 1.1  1994/04/21  10:07:50  habr
# Initial revision
#
#
#
#
# Copyright (c) ABB Robotics AB 1991  All rights reserved
#
############################################################################## 
#
# Text resource number = 52?? 
72::
#
# Reference to system internal ReaL-class (do not translate)
0:
rlraps
# Type of top object  : DATA TYPE
# Ref. to top object  : num
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
1:
num
# Type of top object  : DATA TYPE
# Ref. to top object  : num
# Type of text object : DATA TYPE
# Full name.......... : SYMbolic NUMeric
# Note............... :
2:
symnum
# Type of top object  : INSTRUCTION
# Ref. to top object  : OpMode
# Type of text object : INSTRUCTION
# Full name.......... : OPerating MODE
# Note............... : 
3:
OpMode
# Type of top object  : INSTRUCTION
# Ref. to top object  : RunMode
# Type of text object : INSTRUCTION
# Full name.......... : RUNning MODE
# Note............... : 
4:
RunMode
# Type of top object  : INSTRUCTION
# Ref. to top object  : ErrWrite
# Type of text object : INSTRUCTION
# Full name.......... : Error Write
# Note............... : 
5:
ErrWrite
# Type of top object  : INSTRUCTION
# Ref. to top object  : ErrWrite
# Type of text object : SWITCH PARAMETER 
# Full name.......... : Warning
# Note............... : 
6:
W
# Type of top object  : DATA TYPE
# Ref. to top object  : switch
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
7:
switch
# Type of top object  : DATA TYPE
# Ref. to top object  : string
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
8:
string
# Type of top object  : INSTRUCTION
# Ref. to top object  : ErrWrite
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Header
# Note............... : 
9:
Header
# Type of top object  : INSTRUCTION
# Ref. to top object  : ErrWrite
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Reason
# Note............... : 
10:
Reason
# Type of top object  : INSTRUCTION
# Ref. to top object  : ErrWrite
# Type of text object : OPTION PARAMETER 
# Full name.......... : RL2
# Note............... : 
11:
RL2
# Type of top object  : INSTRUCTION
# Ref. to top object  : ErrWrite
# Type of text object : OPTION PARAMETER 
# Full name.......... : RL3
# Note............... : 
12:
RL3
# Type of top object  : INSTRUCTION
# Ref. to top object  : ErrWrite
# Type of text object : OPTION PARAMETER 
# Full name.......... : RL4
# Note............... : 
13:
RL4
# Type of top object  : DATA TYPE
# Ref. to top object  : signaldo
# Type of text object : DATA TYPE
# Full name.......... : SIGNAL Digital Output
# Note............... : Reference to already installed type name.
14:
signaldo
# Type of top object  : INSTRUCTION
# Ref. to top object  : PFDOVal, PFGOVal
# Type of text object : REQUIRED PARAMETER
# Full name.......... : SIGNAL
# Note............... :
15:
Signal
# Type of top object  : DATA TYPE
# Ref. to top object  : num
# Type of text object : DATA TYPE
# Full name.......... : Digital Input and Output Numeric
# Note............... : Reference to already installed type name.
16:
dionum
# Type of top object  : INSTRUCTION
# Ref. to top object  : PFDOVal
# Type of text object : INSTRUCTION
# Full name.......... : Power Failure Digital Output VALue
# Note............... : 
17:
PFDOVal
# Type of top object  : DATA TYPE
# Ref. to top object  : signalgo
# Type of text object : DATA TYPE
# Full name.......... : SIGNAL Group of digital Outputs
# Note............... : Reference to already installed type name.
18:
signalgo
# Type of top object  : INSTRUCTION
# Ref. to top object  : PFGOVal
# Type of text object : INSTRUCTION
# Full name.......... : Power Failure Group Output VALue
# Note............... : 
19:
PFGOVal
# Type of top object  : INSTRUCTION
# Ref. to top object  : PFRestart
# Type of text object : SWITCH PARAMETER 
# Full name.......... : BASE
# Note............... : 
20:
Base
# Type of top object  : INSTRUCTION
# Ref. to top object  : PFRestart
# Type of text object : SWITCH PARAMETER 
# Full name.......... : InterRuPT
# Note............... : 
21:
Irpt
# Type of top object  : INSTRUCTION
# Ref. to top object  : PFRestart
# Type of text object : INSTRUCTION
# Full name.......... : Power Failure RESTART
# Note............... : 
22:
PFRestart
# Type of top object  : DATA TYPE
# Ref. to top object  : bool
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
23:
bool
# Type of top object  : INSTRUCTION
# Ref. to top object  : PFIOResto
# Type of text object : INSTRUCTION
# Full name.......... : Power Failure Input Output RESTOre
# Note............... : 
24:
PFIOResto
# Type of top object  : FUNCTION
# Ref. to top object  : TextGet
# Type of text object : FUNCTION
# Full name.......... : TEXTGET
# Note............... : Function for RAPID development (shell routines)
25:
TextGet
# Type of top object  : FUNCTION
# Ref. to top object  : TextGet
# Type of text object : REQUIRED PARAMETER
# Full name.......... : TABLE
# Note............... : 
26:
Table
# Type of top object  : FUNCTION
# Ref. to top object  : TextGet
# Type of text object : REQUIRED PARAMETER
# Full name.......... : INDEX
# Note............... : 
27:
Index
# Type of top object  : FUNCTION
# Ref. to top object  : ArgName
# Type of text object : FUNCTION
# Full name.......... : ARGument NAME
# Note............... : 
28:
ArgName
# Type of top object  : FUNCTION
# Ref. to top object  : ArgName
# Type of text object : REQUIRED PARAMETER
# Full name.......... : PARAMETER
# Note............... : 
29:
Parameter
# Type of top object  : DATA TYPE
# Ref. to top object  : errnum
# Type of text object : DATA TYPE
# Full name.......... : ERRor NUMeric
# Note............... : 
30:
errnum
# INTERNAL SYSTEM USE
# DO NOT TRANSLATE OR CHANGE ANYTHING FOR TEXT NO 31
31:
ANYTYPE#
# Type of top object  : FUNCTION
# Ref. to top object  : TextTabGet
# Type of text object : FUNCTION
# Full name.......... : TEXT TABLE GET
# Note............... : Function for RAPID development (shell routines)
32:
TextTabGet
# Type of top object  : FUNCTION
# Ref. to top object  : TextTabGet
# Type of text object : REQUIRED PARAMETER
# Full name.......... : TABLE NAME
# Note............... : 
33:
TableName
# Type of top object  : INSTRUCTION
# Ref. to top object  : BookErrNo
# Type of text object : INSTRUCTION
# Full name.......... : BOOK ERRor Number
# Note............... : Instruction for RAPID development (shell routines)
34:
BookErrNo
# Type of top object  : INSTRUCTION
# Ref. to top object  : BookErrNo
# Type of text object : REQUIRED PARAMETER
# Full name.......... : ERROR NAME
# Note............... : 
35:
ErrorName
# Type of top object  : FUNCTION
# Ref. to top object  : IsOptId
# Type of text object : REQUIRED PARAMETER
# Full name.......... : IS OPTion ID present
# Note............... : 
36:
IsOptId
# Type of top object  : FUNCTION
# Ref. to top object  : IsOptId
# Type of text object : REQUIRED PARAMETER
# Full name.......... : Option Identity
# Note............... : 
37:
OptionId
# Type of top object  : FUNCTION
# Ref. to top object  : IsSysId
# Type of text object : REQUIRED PARAMETER
# Full name.......... : IS SYStem ID present
# Note............... : 
38:
IsSysId
# Type of top object  : FUNCTION
# Ref. to top object  : IsSysId
# Type of text object : REQUIRED PARAMETER
# Full name.......... : System Identity
# Note............... : 
39:
SystemId

# Type of top object  : INSTRUCTION
# Ref. to top object  : SkipWarn
# Type of text object : INSTRUCTION
# Full name.......... : Skip latest elog warning
# Note............... : 
40:
SkipWarn

# Type of top object  : FUNCTION
# Ref. to top object  : SingAreaWrist
# Type of text object : FUNCTION
# Full name.......... : SINGular AREA WRIST
# Note............... : 
41:
SingAreaWrist

# Type of top object  : FUNCTION
# Ref. to top object  : RunMode
# Type of text object : OPTION PARAMETER
# Full name.......... : MAIN program task
# Note............... : 
42:
Main

# Type of top object  : INSTRUCTION
# Ref. to top object  : BookErrNo
# Type of text object : INSTRUCTION
# Full name.......... : BOOK ERRor Number
# Note............... : Hidden and secret for LoadId
43:
BookErrNo_x43

# Type of top object  : FUNCTION
# Ref. to top object  : TextTabGet
# Type of text object : FUNCTION
# Full name.......... : TEXT TABle GET
# Note............... : Hidden and secret for LoadId
44:
TextTabGet_x44

# Type of top object  : FUNCTION
# Ref. to top object  : TextGet
# Type of text object : FUNCTION
# Full name.......... : TEXTGET
# Note............... : Hidden and secret for LoadId
45:
TextGet_x45

# Type of top object  : FUNCTION
# Ref. to top object  : ArgName
# Type of text object : FUNCTION
# Full name.......... : ARGument NAME
# Note............... : Hidden and secret for LoadId
46:
ArgName_x46

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : 
47:
restartdata

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... :
# Note............... : 
48:
stoponpath

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
49:
predo1val

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
50:
postdo1val

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
51:
prego1val

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
52:
postgo1val

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
53:
prego2val

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
54:
postgo2val

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
55:
prego3val

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
56:
postgo3val

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
57:
prego4val

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
58:
postgo4val

# Type of top object  : INSTRUCTION
# Ref. to top object  : TriggStopProc
# Type of text object : INSTRUCTION
# Full name.......... : 
# Note............... : 
59:
TriggStopProc

# Type of top object  : INSTRUCTION
# Ref. to top object  : TriggStopProc
# Type of text object : REQUIRED PARAMETER
# Full name.......... : 
# Note............... : 
60:
RestartRef

# Type of top object  : INSTRUCTION
# Ref. to top object  : TriggStopProc
# Type of text object : OPTION PARAMETER
# Full name.......... : 
# Note............... : 
61:
DO1

# Type of top object  : INSTRUCTION
# Ref. to top object  : TriggStopProc
# Type of text object : OPTION PARAMETER
# Full name.......... : 
# Note............... : 
62:
GO1

# Type of top object  : INSTRUCTION
# Ref. to top object  : TriggStopProc
# Type of text object : OPTION PARAMETER
# Full name.......... : 
# Note............... : 
63:
GO2

# Type of top object  : INSTRUCTION
# Ref. to top object  : TriggStopProc
# Type of text object : OPTION PARAMETER
# Full name.......... : 
# Note............... : 
64:
GO3

# Type of top object  : INSTRUCTION
# Ref. to top object  : TriggStopProc
# Type of text object : OPTION PARAMETER
# Full name.......... : 
# Note............... : 
65:
GO4

# Type of top object  : INSTRUCTION
# Ref. to top object  : TriggStopProc
# Type of text object : REQUIRED PARAMETER
# Full name.......... : 
# Note............... : 
66:
ShadowDO

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
67:
restartstop

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
68:
preshadowval

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
69:
shadowflanks

# Type of top object  : DATA TYPE
# Ref. to top object  : restartdata
# Type of text object : DATA COMPONENT
# Full name.......... : 
# Note............... : 
70:
postshadowval

# Type of top object  : INSTRUCTION
# Ref. to top object  : MailSend
# Type of text object : INSTRUCTION
# Full name.......... : MAILSEND
# Note............... : 
71:
MailSend

# Type of top object  : INSTRUCTION
# Ref. to top object  : MailSend
# Type of text object : REQUIRED PARAMETER
# Full name.......... : SENDTO
# Note............... : 
72:
SendTo

# Type of top object  : INSTRUCTION
# Ref. to top object  : MailSend
# Type of text object : REQUIRED PARAMETER
# Full name.......... : SUBJECT
# Note............... : 
73:
Subject

# Type of top object  : INSTRUCTION
# Ref. to top object  : MailSend
# Type of text object : REQUIRED PARAMETER
# Full name.......... : TEXT 1
# Note............... : 
74:
Text1

# Type of top object  : INSTRUCTION
# Ref. to top object  : MailSend
# Type of text object : OPTION PARAMETER
# Full name.......... : Text 2
# Note............... : 
75:
T2

# Type of top object  : INSTRUCTION
# Ref. to top object  : MailSend
# Type of text object : OPTION PARAMETER
# Full name.......... : Text 3
# Note............... : 
76:
T3

# Type of top object  : INSTRUCTION
# Ref. to top object  : MailSend
# Type of text object : OPTION PARAMETER
# Full name.......... : Text 4
# Note............... : 
77:
T4

# Type of top object  : INSTRUCTION
# Ref. to top object  : MailSend
# Type of text object : OPTION PARAMETER
# Full name.......... : Text 5
# Note............... : 
78:
T5

# Type of top object  : INSTRUCTION
# Ref. to top object  : RobOS
# Type of text object : INSTRUCTION
# Full name.......... : ROBot OS
# Note............... : 
79:
RobOS

# Type of top object  : INSTRUCTION
# Ref. to top object  : WarmStart
# Type of text object : INSTRUCTION
# Full name.......... : WARM START
# Note............... : 
80:
WarmStart

# Type of top object  : FUNCTION
# Ref. to top object  : TextTabFreeToUse
# Type of text object : FUNCTION
# Full name.......... : TEXTTABleFREETOUSE
# Note............... : 
81:
TextTabFreeToUse

# Type of top object  : FUNCTION
# Ref. to top object  : TextTabFreeToUse
# Type of text object : REQUIRED PARAMETER
# Full name.......... : TABLENAME
# Note............... : 
82:
TableName

# Type of top object  : INSTRUCTION
# Ref. to top object  : TextTabInstall
# Type of text object : INSTRUCTION
# Full name.......... : TEXTTABleINSTALL
# Note............... : 
83:
TextTabInstall

# Type of top object  : INSTRUCTION
# Ref. to top object  : TextTabInstall
# Type of text object : REQUIRED PARAMETER
# Full name.......... : FILE
# Note............... : 
84:
File

# Type of top object  : FUNCTION
# Ref. to top object  : GetTaskName
# Type of text object : FUNCTION
# Full name.......... : GETTASKNAME
# Note............... : 
85:
GetTaskName

# Type of top object  : FUNCTION
# Ref. to top object  : GetTaskName
# Type of text object : OPTION PARAMETER
# Full name.......... : TASKNO
# Note............... : 
86:
TaskNo

# Type of top object  : FUNCTION
# Ref. to top object  : CSpeedOverride
# Type of text object : FUNCTION
# Full name.......... : Current SPEED OVERRIDE
# Note............... : 
87:
CSpeedOverride

# Type of top object  : FUNCTION
# Ref. to top object  : ProgMemFree
# Type of text object : FUNCTION
# Full name.......... : Program Memory Free
# Note............... : 
88:
ProgMemFree

# Type of top object  : FUNCTION
# Ref. to top object  : GetSysInfo
# Type of text object : FUNCTION
# Full name.......... : Get system information
# Note............... : 
89:
GetSysInfo

# Type of top object  : FUNCTION
# Ref. to top object  : GetSysInfo
# Type of text object : OPTIONAL PARAMETER
# Full name.......... : Serial number
# Note............... : 
90:
SerialNo

# Type of top object  : FUNCTION
# Ref. to top object  : GetSysInfo
# Type of text object : OPTIONAL PARAMETER
# Full name.......... : Software version
# Note............... : 
91:
SWVersion

# Type of top object  : FUNCTION
# Ref. to top object  : GetSysInfo
# Type of text object : OPTIONAL PARAMETER
# Full name.......... : Robot type
# Note............... : 
92:
RobotType
93:
NonMotionMode

# Note: When texts are added, check rlrapser.eng too.
# End of file
