###################################################################
#
# rlio.eng  -  Class rlio english RAPID text description file  
#
# $Revision: 1.9 $
#
# DESCRIPTION:
#
#  ReaL text description file
# 
# DEFINITION AND TRANSLATION RULES
# 
# This file refer to following type of top object in the RAPID (ARL)
# Reference Manual: INSTRUCTION, FUNCTION or DATA TYPE
#
# Following general rules for ARL Identifiers must applies for translation to
# native language of all text objects:
# - Maximum general length of text object 16 characters
# - Characters means letters, digits or underscore _ (According ISO 8859-1)
# - The first character in an text object must be a letter
# - All characters are significant
# - Text object differing only in the use of corresponding upper and lower
#   case letters are considered the same
#
# Type of text objects to translate:
# (1) Name of INSTRUCTION:
#     - Max. 10 characters (Instruction Plock List) 
#     - Upper case letter for the first letter in one word. The rest of the word
#       in lower case letters. Normal abbreviation of several words.
#     - E.g. MoveL for Move Linear
# (2) Name of FUNCTION:
#     - Max. 10 characters. (Instruction Plock List)
#       Need for shorter for expression context.
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters. Normal abbreviation of several words.
#     - E.g. ReadNum for Read Numerical
# 
# (3) Name of REQUIRED PARAMETER:
#     - Must not be short (not in the program list)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. Speed
#
# (4) Name of OPTION PARAMETER:
#     - Must be short (in the program list)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. WObj for Work Object
#
# (5) Name of SWITCH PARAMETER:
#     - Must be short (in the program list)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. Conc for Concurrent
#
# (6) Name of DATA TYPE:
#     - Must not be short (not in the visible program list)
#     - Only lower case letters
#     - E.g. robtarget for robot target
#
# (7) Name of DATA COMPONENT:
#     - Must be short (in the program list)
#     - Only lower case letters
#     - E.g. robconf for robot configuration
#
# MODIFICATIONS:
#
# $Log: rlio.eng,v $
# Revision 1.9  2005/01/24 14:33:35  SE-SIGADMIN
# Patch: seanlag2401H14M14S01 Solved SPR: 1021037 Test status: SY Log: Dengensha Interface;
#
# Revision 1.10  2005/01/24 12:58:59  seanlag
# SPR1021037
# Checked: Embedded
# New texts for new rapid instructions for
# the Dengensha Interface option.
#
# Revision 1.7  2001/12/17 19:00:10  SIGADMIN
# Patch: hajn1612H16M46S51 Solved SPR: 1010088 Test status: SS Log: New RAPID instructions, IODNGetAttr and IODNSetAttr;
#
# Revision 1.8  2001/12/16 15:26:10  hajn
# New RAPID instructions added: IODNGetAttr and IODNSetAttr
#
# Revision 1.7  2000-10-04 12:27:51+02  pihi
# SPR 1007478, new function IofGenInstr.
#
# Revision 1.6  2000-10-03 07:39:14+02  pihi
# SPR 1006866, added optional parameter \sync to instruction SetDO
#
# Revision 1.5  2000-03-14 11:43:24+01  sejo
# Text nr 2-7 and 36 hardcoded in C
#
# Revision 1.4  1999-11-16 11:20:33+01  daki
# IOAssign -> SetIO_x54
#
# Revision 1.3  1999-11-08 15:27:47+01  daki
# Add IOAssign instruction
#
# Revision 1.2  1999-04-26 15:08:59+02  sejo
# SPR-1004575 PulseDO at almost the same time solved by FRFAC
#
# Revision 1.2  1999/04/26  12:10:38  sejo
# SPR-1004575 PulseDO after each other
#
# Revision 1.2  1999/04/21  09:00:04  mibe
# add switch High to PulseDo
#
# Revision 1.1  1999/04/09  11:59:15  mibe
# Initial revision
#
# Revision 1.13  1998/09/12  17:14:21  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol
#
# Revision 1.1  1998/05/06  15:54:17  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.12  1998/05/06  11:26:33  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol
#
# Revision 1.1  1996/11/27  09:27:38  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.11  1996/11/27  08:32:39  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/project2/foxfun/rol/classlib/rlio
#
# Revision 1.4  1996/09/02  09:17:35  krha
# New function AOutput
#
# Revision 1.3  1996/08/27  14:15:57  krha
# Error texts in new .eng file
#
# Revision 1.2  1996/08/27  14:04:08  lahu
# error text for time out inserted.
#
# Revision 1.1  1996/04/09  13:50:09  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.10  1996/04/09  13:25:08  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/project2/foxfun/rol/classlib/rlio
#
# Revision 1.2  1996/04/09  10:00:25  lahu
# new instructions: ioenable, iodisable, aliasio.
#
# Revision 1.1  1995/12/06  13:05:37  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.9  1995/12/06  12:33:23  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/project2/foxfun/rol/classlib/rlio
#
# Revision 1.1  1995/04/12  11:47:05  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.8  1995/04/12  10:21:23  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib/rlio
#
# Revision 1.2  1994/08/16  08:59:34  sejo
# Max. instruction/function length 9 -> 10 characters
#
# Revision 1.1  1994/07/07  15:28:18  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.7  1994/07/07  10:23:03  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib
#
# Revision 1.3  1994/06/07  09:08:05  elhu
# New error messages handling
# Adjusted to new release
#
# Revision 1.2  1994/02/11  14:50:25  elhu
# External types are now text_id not strings.
#
# Revision 1.1  1994/01/09  17:59:11  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.6  1994/01/09  17:54:58  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib/rlio
#
# Revision 1.1  1993/12/30  16:47:22  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.5  1993/12/30  16:42:48  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib/rlio
#
# Revision 1.1  1993/09/28  21:36:45  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.4  1993/09/28  20:42:45  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib
#
# Revision 1.1  1993/06/11  09:19:29  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.3  1993/06/11  09:10:15  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib/rlio
#
# Revision 1.2  1993/05/19  15:57:33  bjan
# "Modified for foxsig 0.5a"
#
#
# $Revision: 1.9 $
#
# Copyright (c) ABB Robotics AB 1991  All rights reserved
#
############################################################################## 
#
# Text resource number = 54 
54::
# Reference to system internal ReaL-class (do not translte)
0:
Class rlio
# Type of top object  : DATA TYPE
# Ref. to top object  : num
# Type of text object : DATA TYPE
# Full name.......... : Digital Input and Output Numeric
# Note............... :
1:
dionum
# Type of top object  : DATA TYPE
# Ref. to top object  : signalai
# Type of text object : DATA TYPE
# Full name.......... : SIGNAL Analog Input
# Note............... : DO NOT CHANGE TEXT NO - HARDCODED IN C CODE
2:
signalai
# Type of top object  : DATA TYPE
# Ref. to top object  : signalao
# Type of text object : DATA TYPE
# Full name.......... : SIGNAL Analog Output
# Note............... : DO NOT CHANGE TEXT NO - HARDCODED IN C CODE
3:
signalao
# Type of top object  : DATA TYPE
# Ref. to top object  : signaldi
# Type of text object : DATA TYPE
# Full name.......... : SIGNAL Digital Input
# Note............... : DO NOT CHANGE TEXT NO - HARDCODED IN C CODE
4:
signaldi
# Type of top object  : DATA TYPE
# Ref. to top object  : signalgi
# Type of text object : DATA TYPE
# Full name.......... : SIGNAL Group of digital Inputs
# Note............... : DO NOT CHANGE TEXT NO - HARDCODED IN C CODE
5:
signalgi
# Type of top object  : DATA TYPE
# Ref. to top object  : signaldo
# Type of text object : DATA TYPE
# Full name.......... : SIGNAL Digital Output
# Note............... : DO NOT CHANGE TEXT NO - HARDCODED IN C CODE
6:
signaldo
# Type of top object  : DATA TYPE
# Ref. to top object  : signalgo
# Type of text object : DATA TYPE
# Full name.......... : SIGNAL Group of digital Outputs
# Note............... : DO NOT CHANGE TEXT NO - HARDCODED IN C CODE
7:
signalgo
# Type of top object  : DATA TYPE
# Ref. to top object  : signalio
# Type of text object : DATA TYPE
# Full name.......... : Not used
# Note............... :
8:
signalio
# Type of top object  : INSTRUCTION
# Ref. to top object  : Set, Reset, InvertDO, PulseDO, SetDO, SetGO, SetAO...
# Type of text object : REQUIRED PARAMETER
# Full name.......... : SIGNAL
# Note............... :
9:
Signal
# Type of top object  : INSTRUCTION
# Ref. to top object  : PulseDO
# Type of text object : OPTION PARAMETER
# Full name.......... : Pulse LENGTH
# Note............... :
10:
PLength
# Type of top object  : INSTRUCTION
# Ref. to top object  : SetDO
# Type of text object : OPTION PARAMETER
# Full name.......... : Signal DELAY
# Note............... :
11:
SDelay
# Type of top object  : INSTRUCTION
# Ref. to top object  : SetDO, SetGO, SetAO
# Type of text object : REQUIRED PARAMETER
# Full name.......... : VALUE
# Note............... :
12:
Value
# Type of top object  : Not used
# Ref. to top object  :
# Type of text object : 
# Full name.......... : 
# Note............... :
13:
name
# Type of top object  : INSTRUCTION
# Ref. to top object  : Set
# Type of text object : INSTRUCTION
# Full name.......... : SET
# Note............... :
14:
Set
# Type of top object  : INSTRUCTION
# Ref. to top object  : Reset
# Type of text object : INSTRUCTION
# Full name.......... : RESET
# Note............... :
15:
Reset
# Type of top object  : INSTRUCTION
# Ref. to top object  : InvertDO
# Type of text object : INSTRUCTION
# Full name.......... : Invert Digital Output
# Note............... :
16:
InvertDO
# Type of top object  : INSTRUCTION
# Ref. to top object  : PulseDO
# Type of text object : INSTRUCTION
# Full name.......... : PULSE Digital Output
# Note............... :
17:
PulseDO
# Type of top object  : INSTRUCTION
# Ref. to top object  : SetDO
# Type of text object : INSTRUCTION
# Full name.......... : Set Digital Output
# Note............... :
18:
SetDO
# Type of top object  : INSTRUCTION
# Ref. to top object  : SetGO
# Type of text object : INSTRUCTION
# Full name.......... : Set Group of Digital Output
# Note............... :
19:
SetGO
# Type of top object  : INSTRUCTION
# Ref. to top object  : SetAO
# Type of text object : INSTRUCTION
# Full name.......... : Set Analog Output
# Note............... :
20:
SetAO
# Type of top object  : INSTRUCTION
# Ref. to top object  : DInput
# Type of text object : INSTRUCTION
# Full name.......... : Digital INPUT
# Note............... :
21:
DInput
# Type of top object  : INSTRUCTION
# Ref. to top object  : GInput
# Type of text object : INSTRUCTION
# Full name.......... : Group of digital INPUTs
# Note............... :
22:
GInput
# Type of top object  : INSTRUCTION
# Ref. to top object  : DOutput
# Type of text object : INSTRUCTION
# Full name.......... : Digital OUTPUT
# Note............... :
23:
DOutput
# Type of top object  : INSTRUCTION
# Ref. to top object  : GOutput
# Type of text object : INSTRUCTION
# Full name.......... : Group of digital OUTPUTs
# Note............... :
24:
GOutput
# Type of top object  : INSTRUCTION
# Ref. to top object  : AInput
# Type of text object : INSTRUCTION
# Full name.......... : Analog INPUT
# Note............... :
25:
AInput
# Type of top object  : DATA TYPE
# Ref. to top object  : num
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
26:
num

# Type of top object  : INSTRUCTION
# Ref. to top object  : IOEnable
# Type of text object : INSTRUCTION
# Full name.......... : IO ENABLE
# Note............... :
32:
IOEnable
# Type of top object  : INSTRUCTION
# Ref. to top object  : IODisable
# Type of text object : INSTRUCTION
# Full name.......... : IO DISABLE
# Note............... :
33:
IODisable
# Type of top object  : INSTRUCTION
# Ref. to top object  : IOEnable IODisable
# Type of text object : REQUIRED PARAMETER
# Full name.......... : Unit Name
# Note............... :
34:
UnitName
# Type of top object  : INSTRUCTION
# Ref. to top object  : IOEnable IODisable
# Type of text object : REQUIRED PARAMETER
# Full name.......... : Max Time
# Note............... :
35:
MaxTime
# Type of top object  : DATA TYPE
# Ref. to top object  : string
# Type of text object : DATA TYPE
# Full name.......... : 
# Note............... : Reference to already installed type name.
# Note................: DO NOT CHANGE TEXT NO - HARDCODED IN C CODE
36:
string
# Type of top object  : DATA TYPE
# Ref. to top object  : errnum
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
37:
errnum
# Type of top object  : INSTRUCTION
# Ref. to top object  : AliasIO
# Type of text object : INSTRUCTION
# Full name.......... : Alias IO
# Note............... :
38:
AliasIO
# INTERNAL SYSTEM USE
# DO NOT TRANSLATE OR CHANGE ANYTHING FOR TEXT NO 39
39:
ANYTYPE#
# Type of top object  : INSTRUCTION
# Ref. to top object  : AliasIO
# Type of text object : REQUIRED PARAMETER
# Full name.......... : From Signal
# Note............... :
40:
FromSignal
# Type of top object  : INSTRUCTION
# Ref. to top object  : AliasIO
# Type of text object : REQUIRED PARAMETER
# Full name.......... : To Signal
# Note............... :
41:
ToSignal
# Type of top object  : INSTRUCTION
# Ref. to top object  : AOutput
# Type of text object : INSTRUCTION
# Full name.......... : Analog Output
# Note............... :
45:
AOutput
# Type of top object  : INSTRUCTION
# Ref. to top object  : PulseDO
# Type of text object : SWITCH PARAMETER
# Full name.......... : High
# Note............... :
52:
High
# Type of top object  : DATA TYPE
# Ref. to top object  : switch
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
53:
switch
# Type of top object  : INSTRUCTION
# Ref. to top object  : SetIO_x54
# Type of text object : INSTRUCTION
# Full name.......... : Set IO even if it is protected
54:
SetIO_x54

# Type of top object  : INSTRUCTION
# Ref. to top object  : SetDO
# Type of text object : SWITCH PARAMETER
# Full name.......... : SYNChronize
# Note............... :
55:
Sync

# Type of top object  : INSTRUCTION
# Ref. to top object  : IofGenInstr
# Type of text object : INSTRUCTION 
# Full name.......... : IOF GENerell INSTruction
# Note............... : 
57:
IofGenInstr

# Type of top object  : DATA TYPE
# Ref. to top object  : iofgendata
# Type of text object : DATA COMPONENT 
# Full name.......... : 
# Note............... : 
58:
value1

# Type of top object  : DATA TYPE
# Ref. to top object  : iofgendata
# Type of text object : DATA COMPONENT 
# Full name.......... : 
# Note............... : 
59:
value2

# Type of top object  : DATA TYPE
# Ref. to top object  : iofgendata
# Type of text object : DATA COMPONENT 
# Full name.......... : 
# Note............... : 
60:
value3

# Type of top object  : DATA TYPE
# Ref. to top object  : iofgendata
# Type of text object : DATA COMPONENT 
# Full name.......... : 
# Note............... : 
61:
value4

# Type of top object  : DATA TYPE
# Ref. to top object  : iofgendata
# Type of text object : DATA COMPONENT 
# Full name.......... : 
# Note............... : 
62:
value5

# Type of top object  : DATA TYPE
# Ref. to top object  : iofgendata
# Type of text object : DATA COMPONENT 
# Full name.......... : 
# Note............... : 
63:
value6

# Type of top object  : DATA TYPE
# Ref. to top object  : iofgendata
# Type of text object : DATA COMPONENT 
# Full name.......... : 
# Note............... : 
64:
string1

# Type of top object  : DATA TYPE
# Ref. to top object  : iofgendata
# Type of text object : DATA COMPONENT 
# Full name.......... : 
# Note............... : 
65:
string2

# Type of top object  : INSTRUCTION
# Ref. to top object  : IofGenInstr
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : 
# Note............... : 
66:
Instruction

# Type of top object  : DATA TYPE
# Ref. to top object  : MocGenInstr
# Type of text object : DATA TYPE
# Full name.......... : IOF GENerel DATA
# Note............... : 
67:
iofgendata

# Type of top object  : INSTRUCTION
# Ref. to top object  : IofGenInstr
# Type of text object : REQUIRED PARAMETER
# Full name.......... : 
# Note............... : 
68:
Data

# Type of top object  : INSTRUCTION
# Ref. to top object  : IODNGetAttr
# Type of text object : INSTRUCTION
# Full name.......... : In/Out DeviceNet Get Attribute
# Note............... : 
69:
IODNGetAttr

# Type of top object  : INSTRUCTION
# Ref. to top object  : IODNSetAttr
# Type of text object : INSTRUCTION
# Full name.......... : In/Out DeviceNet Set Attribute
# Note............... : 
70:
IODNSetAttr

# Type of top object  : INSTRUCTION
# Ref. to top object  : IODNGetAttr, IODNSetAttr
# Type of text object : REQUIRED PARAMETER
# Full name.......... : 
# Note............... : 
71:
UnitName

# Type of top object  : INSTRUCTION
# Ref. to top object  : IODNGetAttr, IODNSetAttr
# Type of text object : REQUIRED PARAMETER
# Full name.......... : 
# Note............... : 
72:
Path

# Type of top object  : INSTRUCTION
# Ref. to top object  : IODNSetAttr
# Type of text object : REQUIRED PARAMETER
# Full name.......... :
# Note............... : 
73:
SetValue

# Type of top object  : INSTRUCTION
# Ref. to top object  : IODNGetAttr
# Type of text object : REQUIRED PARAMETER
# Full name.......... : 
# Note............... : 
74:
GetValue

# Type of top object  : INSTRUCTION
# Ref. to top object  : IODNGetAttr, IODNSetAttr
# Type of text object : OPTIONAL PARAMETER
# Full name.......... : 
# Note............... : 
75:
Timeout

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMReadByte, DPMReadWord, DPMReadLong, DPMWriteByte
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Register index
# Note............... : 
76:
RegIndex

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMReadByte
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Read Byte (Dengensha) 
# Note............... : 
77:
DPMReadByte

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMReadWord
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Read Word (Dengensha) 
# Note............... : 
78:
DPMReadWord

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMReadLong
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Read Long (Dengensha) 
# Note............... : 
79:
DPMReadLong

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWriteByte
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Write Byte(Dengensha) 
# Note............... : 
80:
DPMWriteByte

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWriteByte, DPMWriteWord, DPMWriteLong...
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Register value
# Note............... : 
81:
RegVal

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWriteWord
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Write Word(Dengensha) 
# Note............... : 
82:
DPMWriteWord

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWriteLong
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Write Long(Dengensha) 
# Note............... : 
83:
DPMWriteLong

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMReadStr,DPMWriteStr
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Length in bytes
# Note............... : 
84:
Length

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMReadStr
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Read String(Dengensha) 
# Note............... : 
85:
DPMReadStr

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWriteStr
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Write String(Dengensha) 
# Note............... : 
86:
DPMWriteStr

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWriteStr
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : String to write
# Note............... : 
87:
InputStr

# Type of top object  : DATA TYPE
# Ref. to top object  : Anytype
# Type of text object : DATA TYPE
# Full name.......... : Reference to already installed type name.
# Note............... : 
88:
ANYTYPE#

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWriteBytes
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Write Bytes(Dengensha) 
# Note............... : 
89:
DPMWriteBytes

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWriteWords
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Write Words(Dengensha) 
# Note............... : 
90:
DPMWriteWords

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWriteLongs
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Write Longs(Dengensha) 
# Note............... : 
91:
DPMWriteLongs

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMReadBytes
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Read Bytes(Dengensha) 
# Note............... : 
92:
DPMReadBytes

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMReadWords
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Read Words(Dengensha) 
# Note............... : 
93:
DPMReadWords

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMReadLongs
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Read Longs(Dengensha) 
# Note............... : 
94:
DPMReadLongs

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWatchAdd
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Watch Add(Dengensha) 
# Note............... : 
95:
DPMWatchAdd

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWatchAdd
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Is specific
# Note............... : 
96:
IsSpecific

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWatchAdd
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Specific value
# Note............... : 
97:
SpecVal

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWatchDel
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Watch Del(Dengensha) 
# Note............... : 
98:
DPMWatchDel

# Type of top object  : INSTRUCTION
# Ref. to top object  : DPMWatchDelAll
# Type of text object : INSTRUCTION 
# Full name.......... : Dual Port Memory Watch Del All(Dengensha) 
# Note............... : 
99:
DPMWatchDelAll

# Type of top object  : DATA TYPE
# Ref. to top object  : num
# Type of text object : DATA TYPE
# Full name.......... : Bus state
# Note............... :
100:
busstate

# Type of top object  : INSTRUCTION
# Ref. to top object  : IOBusState
# Type of text object : INSTRUCTION
# Full name.......... : IO Bus State
# Note............... :
101:
IOBusState

# Type of top object  : INSTRUCTION
# Ref. to top object  : IOBusState
# Type of text object : REQUIRED PARAMETER
# Full name.......... : Bus Name
# Note............... :
102:
BusName

# Type of top object  : INSTRUCTION
# Ref. to top object  : IOBusState
# Type of text object : REQUIRED PARAMETER
# Full name.......... : State
# Note............... :
103:
State

# Note: When texts are added, check rlioer.eng too.
# End of file
