###################################################################
#
# rlcom.eng  -  Class rlcom english RAPID text description file  
#
# $Revision: 1.5 $
#
# DESCRIPTION:
#
#  ReaL text description file
# 
# DEFINITION AND TRANSLATION RULES
# 
# This file refer to following type of top object in the RAPID (ARL)
# Reference Manual: INSTRUCTION, FUNCTION or DATA TYPE
#
# Following general rules for ARL Identifiers must applies for translation to
# native language of all text objects:
# - Maximum general length of text object 16 characters
# - Characters means letters, digits or underscore _ (According ISO 8859-1)
# - The first character in an text object must be a letter
# - All characters are significant
# - Text object differing only in the use of corresponding upper and lower
#   case letters are considered the same
#
# Type of text objects to translate:
# (1) Name of INSTRUCTION:
#     - Max. 10 characters (Instruction Plock List) 
#     - Upper case letter for the first letter in one word. The rest of the word
#       in lower case letters. Normal abbreviation of several words.
#     - E.g. MoveL for Move Linear
# (2) Name of FUNCTION:
#     - Max. 10 characters. (Instruction Plock List)
#       Need for shorter for expression context.
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters. Normal abbreviation of several words.
#     - E.g. ReadNum for Read Numerical
# 
# (3) Name of REQUIRED PARAMETER:
#     - Must not be short (not in the program list)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. Speed
#
# (4) Name of OPTION PARAMETER:
#     - Must be short (in the program list)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. WObj for Work Object
#
# (5) Name of SWITCH PARAMETER:
#     - Must be short (in the program list)
#     - Upper case letter for the first letter in the word. The rest of the word
#       in lower case letters.
#     - E.g. Conc for Concurrent
#
# (6) Name of DATA TYPE:
#     - Must not be short (not in the visible program list)
#     - Only lower case letters
#     - E.g. robtarget for robot target
#
# (7) Name of DATA COMPONENT:
#     - Must be short (in the program list)
#     - Only lower case letters
#     - E.g. robconf for robot configuration
#
# MODIFICATIONS:
#
# $Log: rlcom.eng,v $
# Revision 1.5  2003/08/22 16:00:20  SIGADMIN
# Patch: inre2208H16M10S54 Solved SPR: 1001249 Test status: SY Log: A new variant of tpreadfk (tpreadkey) that handle more tp keys;
#
# Revision 1.5  2003/08/22 14:06:10  inre
# SPR:1001249
# Checked: pamu
# Add a new funktion for tpreadfk called tpreadkey that handle more keys
#
# Revision 1.4  2002-05-27 08:52:06+02  hesve
# SPR-1010838 ClearIOBuff available in all system with secret name
#
# Revision 1.3  2002-05-07 16:43:44+02  sejo
# SPR-1010838 Open, Close, WriteBin, ReadBin available in all system with secret name
#
# Revision 1.2  2001-12-11 11:07:18+01  pihi
# Moved CopyFile from class rlfsta
#
# Revision 1.1  1998-09-14 12:30:37+02  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.13  1998/09/12  17:12:45  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol
#
# Revision 1.2  1998/08/17  18:29:57  roda
# Merging files from FRFAC/mibe for rel3.20
#
# Revision 1.3  1998/07/07  17:38:02  mibe
# Fixing of SPRs:
#  SPR-960851 : test of iodev=0 when opening a file
#  SPR-960852 : Open request gives a new file descriptor
#  SPR-1000511: Open a binary file with \Read, \Write or \Append mode
#  SPR-1000511: Allow ReadBin to read bytes from a text file
#  SPR-1000382: ReadStr possibly removes CR character
#  SPR 951549 : ReadStr and ReadNum with possibility to program delimiters
#
# Revision 1.2  1998/05/20  14:48:08  mibe
# add ReadStrBin ReadAnyBin WriteAnyBin and ClearIOBuff
# Revision 1.1  1998/05/06  15:43:30  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.1  1997/07/25  08:49:37  sigadmin
# Initial revision
# Revision 1.12  1998/05/06  11:25:02  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol
#
# Revision 1.2  1997/01/09  15:30:57  sejo
# Corr. of tpnum
#
# Revision 1.1  1996/11/27  09:19:08  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.11  1996/11/27  08:23:28  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/project2/foxfun/rol/classlib/rlcom
#
# Revision 1.8  1996/11/26  15:59:38  lahu
# symnum (rlraps) changed to tpnum.
#
# Revision 1.7  1996/11/25  15:49:07  lahu
# hct manuell vw rel3.0 ok
#
# Revision 1.6  1996/08/27  13:58:47  krha
# Error texts in new .eng file
#
# Revision 1.5  1996/08/27  13:35:56  lahu
# symnum inserted.
#
# Revision 1.4  1996/08/15  13:45:54  lahu
# Indata check WriteBin outside 0-255 S961007. no hptest.
#
# Revision 1.3  1996/05/13  13:01:36  lahu
# flush, rewind and eofile inserted.
#
# Revision 1.2  1996/05/02  09:37:55  lahu
# WriteStrBin inserted.
#
# Revision 1.1  1996/04/09  13:49:37  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.10  1996/04/09  13:24:09  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/project2/foxfun/rol/classlib/rlcom
#
# Revision 1.5  1996/02/22  14:30:27  sejo
# Adjust text for SYS_ERR_ARL_TYPEERR
#
# Revision 1.4  1996/01/25  10:53:32  inre
# *** empty log message ***
#
# Revision 1.3  1996/01/22  13:40:41  inre
# Patch: inre2201H14M39S50  Solved SPR: S951495 S960035 Test status: CL Log: readbin loss of char
#
# Revision 1.2  1995/12/21  16:01:54  lahu
# String too long inserted.
#
# Revision 1.1  1995/12/06  13:05:03  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.9  1995/12/06  12:31:08  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/project2/foxfun/rol/classlib/rlcom
#
# Revision 1.4  1995/11/29  15:31:47  sejo
# Add text id 66 for Text
#
# Revision 1.3  1995/11/29  14:12:19  sejo
# Text ID 8: String -> Str_ing temp. due to bug in pgm
#
# Revision 1.2  1995/06/06  14:42:26  inre
# S950599, better error text and code if the received data is of
# wrong type
#
# Revision 1.1  1995/04/12  11:46:29  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.8  1995/04/12  10:10:08  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib/rlcom
#
# Revision 1.3  1994/09/22  11:56:43  sejo
# Add text TP_Read_Num and TP_Read_FK
#
# Revision 1.2  1994/08/16  08:54:36  sejo
# Max. instruction/function length 9 -> 10 characters
#
# Revision 1.1  1994/07/07  11:37:06  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.7  1994/07/07  10:22:19  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib
#
# Revision 1.6  1994/06/22  12:59:15  elhu
# New break flag on the tp_read functions
#
# Revision 1.5  1994/06/07  09:18:50  elhu
# New error messages handling
# Adjusted to new release
#
# Revision 1.4  1994/03/23  14:37:37  inre
# tpread requests has now a DIBreak and timeout flag.
#
# Revision 1.3  1994/03/15  07:11:51  inre
# S940241 change request implemented ( TPRead.. -> to procedure )
#
# Revision 1.2  1994/02/11  14:44:02  elhu
# External types are now text_id not strings.
#
# Revision 1.1  1994/01/09  17:34:43  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.6  1994/01/09  17:31:21  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib/rlcom
#
# Revision 1.1  1993/12/30  17:07:10  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.5  1993/12/30  17:05:34  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib/rlcom
#
# Revision 1.1  1993/09/28  21:24:07  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.4  1993/09/28  20:41:07  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib
#
# Revision 1.3  1993/09/09  07:43:08  inre
# Updated to 0.7
#
# Revision 1.2  1993/06/17  08:47:17  svenej
# "Tp -> TP in all instruction name.
# Parameter name IoDevice -> IODevice"
#
# Revision 1.1  1993/06/11  08:54:07  roladmin
# Initial revision\
# ^^^^^^^^^^^^ PROJECT COMMENTS BEGIN ^^^^^^^^^^^^^
#
# Revision 1.3  1993/06/11  08:49:39  roladmin
# vvvvvvvvvvvv PROJECT COMMENTS END vvvvvvvvvvvv\
# Moved back to subject from/projects/foxfun/rol/classlib/rlcom
#
# Revision 1.2  1993/04/14  08:21:01  bjan
# "New textfile format"
#
# $Revision: 1.5 $
#
#
# Copyright (c) ABB Robotics AB 1991  All rights reserved
#
############################################################################## 
#
# Text resource number = 55 
55::
#
# Type of top object  : 
# Ref. to top object  : 
# Type of text object : 
# Full name.......... : 
# Note............... :
0:
Class rlcom
# Type of top object  : DATA TYPE
# Ref. to top object  : IODEV
# Type of text object : DATA TYPE
# Full name.......... : IO DEVice
# Note............... :
1:
iodev
# Type of top object  : INSTRUCTION
# Ref. to top object  : Open
# Type of text object : REQUIRED PARAMETER
# Full name.......... : file DEVICE
# Note............... : eg "c:\my_dir"
2:
Object
# Type of top object  : INSTRUCTION
# Ref. to top object  : Open
# Type of text object : OPTION PARAMETER 
# Full name.......... : FILE name
# Note............... : 
3:
File
# Type of top object  : INSTRUCTION
# Ref. to top object  : Open
# Type of text object : SWITCH PARAMETER 
# Full name.......... : READ mode
# Note............... : 
4:
Read
# Type of top object  : INSTRUCTION
# Ref. to top object  : Open
# Type of text object : SWITCH PARAMETER 
# Full name.......... : WRITE mode
# Note............... : 
5:
Write
# Type of top object  : INSTRUCTION
# Ref. to top object  : Open
# Type of text object : SWITCH PARAMETER 
# Full name.......... : APPEND mode
# Note............... : 
6:
Append
# Type of top object  : INSTRUCTION
# Ref. to top object  : Open
# Type of text object : SWITCH PARAMETER 
# Full name.......... : BINary mode
# Note............... : 
7:
Bin
# Type of top object  : INSTRUCTION
# Ref. to top object  : Write, TPWrite, TPReadFK, TPReadNum, TPReadStr
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : STRING
# Note............... : 
8:
String
# Type of top object  : INSTRUCTION
# Ref. to top object  : Write, TPWrite
# Type of text object : OPTION PARAMETER 
# Full name.......... : NUMeric 
# Note............... : Numeric part of output string
9:
Num
# Type of top object  : INSTRUCTION
# Ref. to top object  : Write, TPWrite
# Type of text object : OPTION PARAMETER 
# Full name.......... : POSition 
# Note............... : Pos part of output string
10:
Pos
# Type of top object  : INSTRUCTION
# Ref. to top object  : Write, TPWrite
# Type of text object : OPTION PARAMETER 
# Full name.......... : ORIENtation 
# Note............... : Orientation part of output string
11:
Orient
# Type of top object  : INSTRUCTION
# Ref. to top object  : Write, TPWrite
# Type of text object : OPTION PARAMETER 
# Full name.......... : BOOLean 
# Note............... : Boolean part of output string
12:
Bool
# Type of top object  : INSTRUCTION
# Ref. to top object  : Write
# Type of text object : SWITCH PARAMETER 
# Full name.......... : NO NEW LINE 
# Note............... : Cancel default newline
13:
NoNewLine
# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadBin
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : TIME out  
# Note............... : 
14:
Time
# Type of top object  : INSTRUCTION
# Ref. to top object  : WriteBin
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : BUFFER  
# Note............... : Output buffer
15:
Buffer
# Type of top object  : INSTRUCTION
# Ref. to top object  : WriteBin
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Number of CHaRacters  
# Note............... : Number of significant characters in output buffer
16:
NChar
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Function Key text 1  
# Note............... : 
17:
FK1
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Function Key text 2  
# Note............... : 
18:
FK2
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Function Key text 3  
# Note............... : 
19:
FK3
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Function Key text 4  
# Note............... : 
20:
FK4
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Function Key text 5  
# Note............... : 
21:
FK5
# Type of top object  : INSTRUCTION
# Ref. to top object  : Open
# Type of text object : INSTRUCTION
# Full name.......... : OPEN file
# Note............... : 
22:
Open
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadStr
# Type of text object : INSTRUCTION
# Full name.......... : Teach Pendant READ STRing
# Note............... : 
23:
TPReadStr
# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadStr
# Type of text object : INSTRUCTION
# Full name.......... : READ STRing 
# Note............... : 
24:
ReadStr
# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadBin
# Type of text object : INSTRUCTION
# Full name.......... : READ BINary
# Note............... : 
25:
ReadBin
# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadNum
# Type of text object : INSTRUCTION
# Full name.......... : READ NUMeric
# Note............... : 
26:
ReadNum
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadNum
# Type of text object : INSTRUCTION
# Full name.......... : Teach Pendant READ NUMeric
# Note............... : 
27:
TPReadNum
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK
# Type of text object : INSTRUCTION
# Full name.......... : Teach Pendant READ Function Key
# Note............... : 
28:
TPReadFK
# Type of top object  : INSTRUCTION
# Ref. to top object  : Close
# Type of text object : INSTRUCTION
# Full name.......... : CLOSE file
# Note............... : 
29:
Close
# Type of top object  : INSTRUCTION
# Ref. to top object  : Write
# Type of text object : INSTRUCTION
# Full name.......... : WRITE text file
# Note............... : 
30:
Write
# Type of top object  : INSTRUCTION
# Ref. to top object  : WriteBin
# Type of text object : INSTRUCTION
# Full name.......... : WRITE BINary file
# Note............... : 
31:
WriteBin
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPWrite
# Type of text object : INSTRUCTION
# Full name.......... : Teach Pendant WRITE
# Note............... : 
32:
TPWrite
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPErase
# Type of text object : INSTRUCTION
# Full name.......... : Teach Pendant ERASE
# Note............... : 
33:
TPErase
# Type of top object  : INSTRUCTION
# Ref. to top object  : Close, Write, Open
# Type of text object : REQUIRED PARAMETER
# Full name.......... : IO DEVICE reference
# Note............... : 
34:
IODevice
# Type of top object  : DATA TYPE
# Ref. to top object  : errnum
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
35:
errnum
# Type of top object  : DATA TYPE
# Ref. to top object  : switch
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
36:
switch
# Type of top object  : DATA TYPE
# Ref. to top object  : pos
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
37:
pos
# Type of top object  : DATA TYPE
# Ref. to top object  : orient
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
38:
orient
# Type of top object  : DATA TYPE
# Ref. to top object  : bool
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
39:
bool
# Type of top object  : DATA TYPE
# Ref. to top object  : num
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
40:
num
# Type of top object  : DATA TYPE
# Ref. to top object  : string
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
41:
string
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK, TPReadNum, TPReadStr
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Answer
# Note............... : 
42:
Answer
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK, TPReadNum, TPReadStr
# Type of text object : OPTIONAL PARAMETER 
# Full name.......... : MaxTime
# Note............... : 
43:
MaxTime
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK, TPReadNum, TPReadStr
# Type of text object : OPTIONAL PARAMETER 
# Full name.......... : DIBreak
# Note............... : 
44:
DIBreak
# Type of top object  : DATA TYPE
# Ref. to top object  : signaldi
# Type of text object : DATA TYPE
# Full name.......... :
# Note............... : Reference to already installed type name.
45:
signaldi

# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK, TPReadNum, TPReadStr
# Type of text object : OPTIONAL PARAMETER 
# Full name.......... : BreakFlag
# Note............... : 
62:
BreakFlag
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadNum
# Type of text object : INSTRUCTION
# Full name.......... : Teach Pendant READ NUMeric
# Note............... : *** Do not translate ***
63:
TP_Read_Num
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK
# Type of text object : INSTRUCTION
# Full name.......... : Teach Pendant READ Function Key
# Note............... : *** Do not translate ***
64:
TP_Read_FK

# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadFK
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : TEXT
# Note............... : Changed from String to Text in RW2.1
66:
Text

# Type of top object  : INSTRUCTION
# Ref. to top object  : WriteStrBin
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : STRING
# Note............... : 
69:
Str
# Type of top object  : INSTRUCTION
# Ref. to top object  : WriteStrBin
# Type of text object : INSTRUCTION
# Full name.......... : WRITE String to BINary file
# Note............... : 
70:
WriteStrBin
# Type of top object  : INSTRUCTION
# Ref. to top object  : Flush
# Type of text object : INSTRUCTION
# Full name.......... : Flush of serial channel.
# Note............... : 
71:
Flush
# Type of top object  : INSTRUCTION
# Ref. to top object  : Rewind
# Type of text object : INSTRUCTION
# Full name.......... : Rewind of ASCII and BINary file
# Note............... : 
72:
Rewind
# Type of top object  : FUNCTION
# Ref. to top object  : EOFile
# Type of text object : FUNCTION
# Full name.......... : Test if end of file
# Note............... : 
73:
EOFile
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPShow
# Type of text object : INSTRUCTION
# Full name.......... : Teach Pendant WRITE
# Note............... : 
74:
TPShow
# Type of top object  : INSTRUCTION
# Ref. to top object  : TPShow
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Window 
# Note............... : Window number to show
75:
Window

# Type of top object  : DATA TYPE
# Ref. to top object  : tpnum
# Type of text object : DATA TYPE
# Full name.......... : Teach Pendant NUMeric
# Note............... :
79:
tpnum

# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadStrBin
# Type of text object : INSTRUCTION
# Full name.......... : Read String Binary
# Note............... : 
81:
ReadStrBin
# Type of top object  : INSTRUCTION
# Ref. to top object  : WriteAnyBin
# Type of text object : INSTRUCTION
# Full name.......... : Write Anytype Binary
# Note............... : 
82:
WriteAnyBin
# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadAnyBin
# Type of text object : INSTRUCTION
# Full name.......... : Read Anytype Binary
# Note............... : 
83:
ReadAnyBin
# Type of top object  : INSTRUCTION
# Ref. to top object  : ClearIOBuff
# Type of text object : INSTRUCTION
# Full name.......... : Clear I/O Buffer
# Note............... : 
84:
ClearIOBuff
# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadStrBin
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : No Of Chars
# Note............... : 
85:
NoOfChars
# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadAnyBin,WriteAnyBin
# Type of text object : REQUIRED PARAMETER 
# Full name.......... : Data
# Note............... : 
86:
Data
# INTERNAL SYSTEM USE
# DO NOT TRANSLATE OR CHANGE ANYTHING FOR TEXT NO 87
87:
ANYTYPE#
# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadStr,ReadNum
# Type of text object : Optional PARAMETER 
# Full name.......... : Delimiters
# Note............... : 
92:
Delim
# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadStr
# Type of text object : switch PARAMETER 
# Full name.......... : Remove Carriage Return
# Note............... : 
93:
RemoveCR
# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadStr
# Type of text object : switch PARAMETER 
# Full name.......... : Discard Heading Delimiters
# Note............... : 
94:
DiscardHeaders
# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : INSTRUCTION
# Full name.......... : Copy a File
# Note............... :
100:
CopyFile
# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : REQUIRED PARAMETER
# Full name.......... : Old File path 
# Note............... :
101:
OldPath
# Type of top object  : INSTRUCTION
# Ref. to top object  : 
# Type of text object : REQUIRED PARAMETER
# Full name.......... : New File Path 
# Note............... :
102:
NewPath
# Type of top object  : INSTRUCTION
# Ref. to top object  : Open
# Type of text object : INSTRUCTION
# Full name.......... : OPEN file
# Note............... : 
103:
Open_x103
# Type of top object  : INSTRUCTION
# Ref. to top object  : Close
# Type of text object : INSTRUCTION
# Full name.......... : CLOSE file
# Note............... : 
104:
Close_x104
# Type of top object  : INSTRUCTION
# Ref. to top object  : ReadBin
# Type of text object : INSTRUCTION
# Full name.......... : READ BINary
# Note............... : 
105:
ReadBin_x105
# Type of top object  : INSTRUCTION
# Ref. to top object  : WriteBin
# Type of text object : INSTRUCTION
# Full name.......... : WRITE BINary file
# Note............... : 
106:
WriteBin_x106
# Type of top object  : INSTRUCTION
# Ref. to top object  : ClearIOBuff
# Type of text object : INSTRUCTION
# Full name.......... : Clear I/O Buffer
# Note............... : 
107:
ClearIOBuff_x107

# Type of top object  : INSTRUCTION
# Ref. to top object  : TPReadKey
# Type of text object : INSTRUCTION
# Full name.......... : Teach Pendant READ Function Key
# Note............... : 
108:
TPReadKey

# Note: When texts are added, check rlcomer.eng too.
# End of file
